FG{ID}

FLEXIBLE GROUP CONDITIONS

Major Source – New Non-Emergency, SI 4SRB ≤ 500 bhp

This template is for new non-emergency, SI RICE 4SRB equal to or less than 500 bhp at a major source. The RICE is new if the date of installation on and after December 19, 2002.

If this template is being used for an ROP Reopening or Renewal, AND the MACT conditions were established in a PTI, the appropriate footnotes which reference enforceability must be added to each applicable condition in the template.

Blue text is guidance or notes on the use of the template. DELETE ALL BLUE TEXT PRIOR TO ISSUING THE FINAL PERMIT OR SUBMITTING IT WITH A PERMIT APPLICATION.

Red text identifies options. Select the option that applies to the source and change the text to black. Delete red text that does not apply and renumber conditions if necessary.

DESCRIPTION

40 CFR Part 63, Subpart ZZZZ - National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines (RICE), located at a major source of HAP emissions, new, spark ignition, 4SRB, non-emergency RICE, less than or equal to 500 brake hp.

Emission Unit(s): {Enter Emission Unit names}

POLLUTION CONTROL EQUIPMENT

{Enter Pollution Control Equipment or NA}

I. EMISSION LIMITS

NA

II. MATERIAL LIMITS

1.	The permittee shall burn only spark ignition fuels in any engine in FG{ID}. (40 CFR 63.6590)

III. PROCESS/OPERATIONAL RESTRICTIONS

NA

IV. DESIGN/EQUIPMENT PARAMETERS

1.	The nameplate capacity of any engine in FG{ID} shall not exceed 500 bhp, as certified by the equipment manufacturer. (40 CFR 63.6590(c)(4))

V. TESTING/SAMPLING

Records shall be maintained on file for a period of five years. (R 336.1213(3)(b)(ii))

NA

VI. MONITORING/RECORDKEEPING

Records shall be maintained on file for a period of five years. (R 336.1213(3)(b)(ii))

NA

VII. REPORTING

Permit Staff – SC VII.1, 2, and 3, references to Rule 213 are ROP only. Remove before putting into a PTI. Renumber as appropriate.

Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. (R 336.1213(3)(c)(ii))

Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be received by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. (R 336.1213(3)(c)(i))

Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be received by March 15 for the previous calendar year. (R 336.1213(4)(c))

VIII. STACK/VENT RESTRICTIONS

NA

IX. OTHER REQUIREMENTS

1.	The permittee shall comply with the provisions of the federal Standards of Performance for New Stationary Sources as specified in 40 CFR Part 60 Subpart A and Subpart JJJJ, as they apply to any engine in FG{ID}. (40 CFR 63.6590)

2.	The permittee shall comply with all applicable provisions of the National Emission Standards for Hazardous Air Pollutants, as specified in 40 CFR Part 63, Subpart A and Subpart ZZZZ, for Stationary Reciprocating Internal Combustion Engines by the initial compliance date. (40 CFR 63.6595, 40 CFR Part 63, Subparts A and ZZZZ)