|  |  |  |
| --- | --- | --- |
|  | **MICHIGAN DEPARTMENT OF ENVIRONMENT, GREAT LAKES, AND ENERGY****AIR QUALITY DIVISION** |  |
| EFFECTIVE DATE: August 10, 2022ISSUED TO**Hutchinson Antivibration Systems Incorporated**State Registration Number (SRN): A9364LOCATED AT600 7th Street, Cadillac, Wexford County, Michigan 49601 |
|  |
| **RENEWABLE OPERATING PERMIT**Permit Number: MI-ROP-A9364-2022Expiration Date: August 10. 2027Administratively Complete ROP Renewal Application Due Between:February 10, 2026 and February 10, 2027This Renewable Operating Permit (ROP) is issued in accordance with and subject to Section 5506(3) of Part 55, Air Pollution Control, of the Natural Resources and Environmental Protection Act, 1994 PA 451, as amended (Act 451). Pursuant to Rule 210(1) of the administrative rules promulgated under Act 451, this ROP constitutes the permittee’s authority to operate the stationary source identified above in accordance with the general conditions, special conditions and attachments contained herein. Operation of the stationary source and all emission units listed in the permit are subject to all applicable future or amended rules and regulations pursuant to Act 451 and the federal Clean Air Act. |

|  |
| --- |
| **SOURCE-WIDE PERMIT TO INSTALL**Permit Number: MI-PTI-A9364-2022This Permit to Install (PTI) is issued in accordance with and subject to Section 5505(1) of Act 451. Pursuant to Rule 214a of the administrative rules promulgated under Act 451, the terms and conditions herein, identified by the underlying applicable requirement citation of Rule 201(1)(a), constitute a federally enforceable PTI. The PTl terms and conditions do not expire and remain in effect unless the criteria of Rule 201(6) are met. Operation of all emission units identified in the PTI is subject to all applicable future or amended rules and regulations pursuant to Act 451 and the federal Clean Air Act. |

Michigan Department of Environment, Great Lakes, and Energy

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Shane Nixon, Cadillac / Gaylord District Supervisor **TABLE OF CONTENTS**

[AUTHORITY AND ENFORCEABILITY 3](#_Toc106882261)

[A. GENERAL CONDITIONS 4](#_Toc106882262)

[Permit Enforceability 4](#_Toc106882263)

[General Provisions 4](#_Toc106882264)

[Equipment & Design 5](#_Toc106882265)

[Emission Limits 5](#_Toc106882266)

[Testing/Sampling 5](#_Toc106882267)

[Monitoring/Recordkeeping 6](#_Toc106882268)

[Certification & Reporting 6](#_Toc106882269)

[Permit Shield 7](#_Toc106882270)

[Revisions 8](#_Toc106882271)

[Reopenings 8](#_Toc106882272)

[Renewals 9](#_Toc106882273)

[Stratospheric Ozone Protection 9](#_Toc106882274)

[Risk Management Plan 9](#_Toc106882275)

[Emission Trading 9](#_Toc106882276)

[Permit to Install (PTI) 10](#_Toc106882277)

[B. SOURCE-WIDE CONDITIONS 11](#_Toc106882278)

[C. EMISSION UNIT SPECIAL CONDITIONS 12](#_Toc106882279)

[EMISSION UNIT SUMMARY TABLE 12](#_Toc106882280)

[EUROLLCOAT 14](#_Toc106882281)

[EURBRMOLDING 16](#_Toc106882282)

[EURBRCUREOVEN 19](#_Toc106882283)

[D. FLEXIBLE GROUP SPECIAL CONDITIONS 22](#_Toc106882284)

[FLEXIBLE GROUP SUMMARY TABLE 22](#_Toc106882285)

[FGAUTODIP 24](#_Toc106882286)

[FGSPRAYMACHINES 26](#_Toc106882287)

[FGRTO 29](#_Toc106882288)

[FGMACTMMMM 34](#_Toc106882289)

[FGRULE287(2)(c) 40](#_Toc106882290)

[FGCOLDCLEANERS 42](#_Toc106882291)

[E. NON-APPLICABLE REQUIREMENTS 45](#_Toc106882292)

[APPENDICES 46](#_Toc106882293)

[Appendix 1. Acronyms and Abbreviations 46](#_Toc106882294)

[Appendix 2. Schedule of Compliance 47](#_Toc106882295)

[Appendix 3. Monitoring Requirements 47](#_Toc106882296)

[Appendix 4. Recordkeeping 47](#_Toc106882297)

[Appendix 5. Testing Procedures 47](#_Toc106882298)

[Appendix 6. Permits to Install 47](#_Toc106882299)

[Appendix 7. Emission Calculations 48](#_Toc106882300)

[Appendix 8. Reporting 48](#_Toc106882301)

# AUTHORITY AND ENFORCEABILITY

For the purpose of this permit, the **permittee** is defined as any person who owns or operates an emission unit at a stationary source for which this permit has been issued. The **department** is defined in Rule 104(d) as the Director of the Michigan Department of Environment, Great Lakes, and Energy (EGLE) or his or her designee.

The permittee shall comply with all specific details in the permit terms and conditions and the cited underlying applicable requirements. All terms and conditions in this ROP are both federally enforceable and state enforceable unless otherwise footnoted. Certain terms and conditions are applicable to most stationary sources for which an ROP has been issued. These general conditions are included in Part A of this ROP. Other terms and conditions may apply to a specific emission unit, several emission units which are represented as a flexible group, or the entire stationary source which is represented as a Source-Wide group. Special conditions are identified in Parts B, C, D and/or the appendices.

In accordance with Rule 213(2)(a), all underlying applicable requirements are identified for each ROP term or condition. All terms and conditions that are included in a PTI are streamlined, subsumed and/or is state-only enforceable will be noted as such.

In accordance with Section 5507 of Act 451, the permittee has included in the ROP application a compliance certification, a schedule of compliance, and a compliance plan. For applicable requirements with which the source is in compliance, the source will continue to comply with these requirements. For applicable requirements with which the source is not in compliance, the source will comply with the detailed schedule of compliance requirements that are incorporated as an appendix in this ROP. Furthermore, for any applicable requirements effective after the date of issuance of this ROP, the stationary source will meet the requirements on a timely basis, unless the underlying applicable requirement requires a more detailed schedule of compliance.

Issuance of this permit does not obviate the necessity of obtaining such permits or approvals from other units of government as required by law.

# A. GENERAL CONDITIONS

## Permit Enforceability

* All conditions in this permit are both federally enforceable and state enforceable unless otherwise noted. **(R 336.1213(5))**
* Those conditions that are hereby incorporated in a state-only enforceable Source-Wide PTI pursuant to Rule 201(2)(d) are designated by footnote one. **(R 336.1213(5)(a), R 336.1214a(5))**
* Those conditions that are hereby incorporated in a federally enforceable Source-Wide PTI pursuant to Rule 201(2)(c) are designated by footnote two. **(R 336.1213(5)(b), R 336.1214a(3))**

## General Provisions

1. The permittee shall comply with all conditions of this ROP. Any ROP noncompliance constitutes a violation of Act 451, and is grounds for enforcement action, for ROP revocation or revision, or for denial of the renewal of the ROP. All terms and conditions of this ROP that are designated as federally enforceable are enforceable by the Administrator of the United States Environmental Protection Agency (USEPA) and by citizens under the provisions of the federal Clean Air Act (CAA). Any terms and conditions based on applicable requirements which are designated as “state-only” are not enforceable by the USEPA or citizens pursuant to the CAA. **(R 336.1213(1)(a))**
2. It shall not be a defense for the permittee in an enforcement action that it would have been necessary to halt or reduce the permitted activity in order to maintain compliance with the conditions of this ROP. **(R 336.1213(1)(b))**
3. This ROP may be modified, revised, or revoked for cause. The filing of a request by the permittee for a permit modification, revision, or termination, or a notification of planned changes or anticipated noncompliance does not stay any ROP term or condition. This does not supersede or affect the ability of the permittee to make changes, at the permittee’s own risk, pursuant to Rule 215 and Rule 216. **(R 336.1213(1)(c))**
4. The permittee shall allow the department, or an authorized representative of the department, upon presentation of credentials and other documents as may be required by law and upon stating the authority for and purpose of the investigation, to perform any of the following activities: **(R 336.1213(1)(d))**
	1. Enter, at reasonable times, a stationary source or other premises where emissions-related activity is conducted or where records must be kept under the conditions of the ROP.
	2. Have access to and copy, at reasonable times, any records that must be kept under the conditions of the ROP.
	3. Inspect, at reasonable times, any of the following:
		1. Any stationary source.
		2. Any emission unit.
		3. Any equipment, including monitoring and air pollution control equipment.
		4. Any work practices or operations regulated or required under the ROP.
	4. As authorized by Section 5526 of Act 451, sample or monitor at reasonable times substances or parameters for the purpose of assuring compliance with the ROP or applicable requirements.
5. The permittee shall furnish to the department, within a reasonable time, any information the department may request, in writing, to determine whether cause exists for modifying, revising, or revoking the ROP or to determine compliance with this ROP. Upon request, the permittee shall also furnish to the department copies of any records that are required to be kept as a term or condition of this ROP. For information which is claimed by the permittee to be confidential, consistent with the requirements of the 1976 PA 442, MCL §15.231 et seq., and known as the Freedom of Information Act, the person may also be required to furnish the records directly to the USEPA together with a claim of confidentiality. **(R 336.1213(1)(e))**
6. A challenge by any person, the Administrator of the USEPA, or the department to a particular condition or a part of this ROP shall not set aside, delay, stay, or in any way affect the applicability or enforceability of any other condition or part of this ROP. **(R 336.1213(1)(f))**
7. The permittee shall pay fees consistent with the fee schedule and requirements pursuant to Section 5522 of Act 451. **(R 336.1213(1)(g))**
8. This ROP does not convey any property rights or any exclusive privilege. **(R 336.1213(1)(h))**

## Equipment & Design

1. Any collected air contaminants shall be removed as necessary to maintain the equipment at the required operating efficiency. The collection and disposal of air contaminants shall be performed in a manner so as to minimize the introduction of contaminants to the outer air. Transport of collected air contaminants in Priority I and II areas requires the use of material handling methods specified in Rule 370(2).2 **(R 336.1370)**
2. Any air cleaning device shall be installed, maintained, and operated in a satisfactory manner and in accordance with the Michigan Air Pollution Control rules and existing law. **(R 336.1910)**

## Emission Limits

1. Unless otherwise specified in this ROP, the permittee shall comply with Rule 301, which states, in part, “Except as provided in Subrules 2, 3, and 4 of this rule, a person shall not cause or permit to be discharged into the outer air from a process or process equipment a visible emission of a density greater than the most stringent of the following:”2 **(R 336.1301(1))**
	1. A 6-minute average of 20% opacity, except for one 6-minute average per hour of not more than 27% opacity.
	2. A limit specified by an applicable federal new source performance standard.

The grading of visible emissions shall be determined in accordance with Rule 303.

1. The permittee shall not cause or permit the emission of an air contaminant or water vapor in quantities that cause, alone or in reaction with other air contaminants, either of the following:
	1. Injurious effects to human health or safety, animal life, plant life of significant economic value, or property.1 **(R 336.1901(a))**
	2. Unreasonable interference with the comfortable enjoyment of life and property.1**(R 336.1901(b))**

## Testing/Sampling

1. The department may require the owner or operator of any source of an air contaminant to conduct acceptable performance tests, at the owner’s or operator’s expense, in accordance with Rule 1001 and Rule 1003, under any of the conditions listed in Rule 1001(1).2 **(R 336.2001)**
2. Any required performance testing shall be conducted in accordance with Rule 1001(2), Rule 1001(3) and Rule 1003. **(R 336.2001(2), R 336.2001(3), R 336.2003(1))**
3. Any required test results shall be submitted to the Air Quality Division (AQD) in the format prescribed by the applicable reference test method within 60 days following the last date of the test. **(R 336.2001(5))**

## Monitoring/Recordkeeping

1. Records of any periodic emission or parametric monitoring required in this ROP shall include the following information specified in Rule 213(3)(b)(i), where appropriate. **(R 336.1213(3)(b))**
	1. The date, location, time, and method of sampling or measurements.
	2. The dates the analyses of the samples were performed.
	3. The company or entity that performed the analyses of the samples.
	4. The analytical techniques or methods used.
	5. The results of the analyses.
	6. The related process operating conditions or parameters that existed at the time of sampling or measurement.
2. All required monitoring data, support information and all reports, including reports of all instances of deviation from permit requirements, shall be kept and furnished to the department upon request for a period of not less than 5 years from the date of the monitoring sample, measurement, report or application. Support information includes all calibration and maintenance records and all original strip-chart recordings, or other original data records, for continuous monitoring instrumentation and copies of all reports required by the ROP. **(R 336.1213(1)(e), R 336.1213(3)(b)(ii))**

## Certification & Reporting

1. Except for the alternate certification schedule provided in Rule 213(3)(c)(iii)(B), any document required to be submitted to the department as a term or condition of this ROP shall contain an original certification by a Responsible Official which state that, based on information and belief formed after reasonable inquiry, the statements and information in the document are true, accurate, and complete. **(R 336.1213(3)(c))**
2. A Responsible Official shall certify to the appropriate AQD District Office and to the USEPA that the stationary source is and has been in compliance with all terms and conditions contained in the ROP except for deviations that have been or are being reported to the appropriate AQD District Office pursuant to Rule 213(3)(c). This certification shall include all the information specified in Rule 213(4)(c)(i) through (v) and shall state that, based on information and belief formed after reasonable inquiry, the statements and information in the certification are true, accurate, and complete. The USEPA address is: USEPA, Air Compliance Data - Michigan, Air and Radiation Division, 77 West Jackson Boulevard, Chicago, Illinois 60604-3507. **(R 336.1213(4)(c))**
3. The certification of compliance shall be submitted annually for the term of this ROP as detailed in the special conditions, or more frequently if specified in an applicable requirement or in this ROP. **(R 336.1213(4)(c))**
4. The permittee shall promptly report any deviations from ROP requirements and certify the reports. The prompt reporting of deviations from ROP requirements is defined in Rule 213(3)(c)(ii) as follows, unless otherwise described in this ROP. **(R 336.1213(3)(c))**
	1. For deviations that exceed the emissions allowed under the ROP, prompt reporting means reporting consistent with the requirements of Rule 912 as detailed in Condition 25. All reports submitted pursuant to this paragraph shall be promptly certified as specified in Rule 213(3)(c)(iii).
	2. For deviations which exceed the emissions allowed under the ROP and which are not reported pursuant to Rule 912 due to the duration of the deviation, prompt reporting means the reporting of all deviations in the semiannual reports required by Rule 213(3)(c)(i). The report shall describe reasons for each deviation and the actions taken to minimize or correct each deviation.
	3. For deviations that do not exceed the emissions allowed under the ROP, prompt reporting means the reporting of all deviations in the semiannual reports required by Rule 213(3)(c)(i). The report shall describe the reasons for each deviation and the actions taken to minimize or correct each deviation.
5. For reports required pursuant to Rule 213(3)(c)(ii), prompt certification of the reports is described in Rule 213(3)(c)(iii) as either of the following: **(R 336.1213(3)(c))**
	1. Submitting a certification by a Responsible Official with each report which states that, based on information and belief formed after reasonable inquiry, the statements and information in the report are true, accurate, and complete.
	2. Submitting, within 30 days following the end of a calendar month during which one or more prompt reports of deviations from the emissions allowed under the ROP were submitted to the department pursuant to Rule 213(3)(c)(ii), a certification by a Responsible Official which states that; “based on information and belief formed after reasonable inquiry, the statements and information contained in each of the reports submitted during the previous month were true, accurate, and complete.” The certification shall include a listing of the reports that are being certified. Any report submitted pursuant to Rule 213(3)(c)(ii) that will be certified on a monthly basis pursuant to this paragraph shall include a statement that certification of the report will be provided within 30 days following the end of the calendar month.
6. Semiannually for the term of the ROP as detailed in the special conditions, or more frequently if specified, the permittee shall submit certified reports of any required monitoring to the appropriate AQD District Office. All instances of deviations from ROP requirements during the reporting period shall be clearly identified in the reports. **(R 336.1213(3)(c)(i))**
7. On an annual basis, the permittee shall report the actual emissions, or the information necessary to determine the actual emissions, of each regulated air pollutant as defined in Rule 212(6) for each emission unit utilizing the emissions inventory forms provided by the department. **(R 336.1212(6))**
8. The permittee shall provide notice of an abnormal condition, start-up, shutdown, or malfunction that results in emissions of a hazardous or toxic air pollutant which continue for more than one hour in excess of any applicable standard or limitation, or emissions of any air contaminant continuing for more than two hours in excess of an applicable standard or limitation, as required in Rule 912, to the appropriate AQD District Office. The notice shall be provided not later than two business days after the start-up, shutdown, or discovery of the abnormal conditions or malfunction. Notice shall be by any reasonable means, including electronic, telephonic, or oral communication. Written reports, if required under Rule 912, must be submitted to the appropriate AQD District Supervisor within 10 days after the start-up or shutdown occurred, within 10 days after the abnormal conditions or malfunction has been corrected, or within 30 days of discovery of the abnormal conditions or malfunction, whichever is first. The written reports shall include all of the information required in Rule 912(5) and shall be certified by a Responsible Official in a manner consistent with the CAA.2 **(R 336.1912)**

## Permit Shield

1. Compliance with the conditions of the ROP shall be considered compliance with any applicable requirements as of the date of ROP issuance if either of the following provisions is satisfied. **(R 336.1213(6)(a)(i), R 336.1213(6)(a)(ii))**
	1. The applicable requirements are included and are specifically identified in the ROP.
	2. The permit includes a determination or concise summary of the determination by the department that other specifically identified requirements are not applicable to the stationary source.

Any requirements identified in Part E of this ROP have been identified as non-applicable to this ROP and are included in the permit shield.

1. Nothing in this ROP shall alter or affect any of the following:
	1. The provisions of Section 303 of the CAA, emergency orders, including the authority of the USEPA under Section 303 of the CAA. **(R 336.1213(6)(b)(i))**
	2. The liability of the owner or operator of this source for any violation of applicable requirements prior to or at the time of this ROP issuance. **(R 336.1213(6)(b)(ii))**
	3. The applicable requirements of the acid rain program, consistent with Section 408(a) of the CAA. **(R 336.1213(6)(b)(iii))**
	4. The ability of the USEPA to obtain information from a source pursuant to Section 114 of the CAA. **(R 336.1213(6)(b)(iv))**
2. The permit shield shall not apply to provisions incorporated into this ROP through procedures for any of the following:
	1. Operational flexibility changes made pursuant to Rule 215. **(R 336.1215(5))**
	2. Administrative Amendments made pursuant to Rule 216(1)(a)(i)-(iv). **(R 336.1216(1)(b)(iii))**
	3. Administrative Amendments made pursuant to Rule 216(1)(a)(v) until the amendment has been approved by the department. **(R 336.1216(1)(c)(iii))**
	4. Minor Permit Modifications made pursuant to Rule 216(2). **(R 336.1216(2)(f))**
	5. State-Only Modifications made pursuant to Rule 216(4) until the changes have been approved by the department. **(R 336.1216(4)(e))**
3. Expiration of this ROP results in the loss of the permit shield. If a timely and administratively complete application for renewal is submitted not more than 18 months, but not less than 6 months, before the expiration date of the ROP, but the department fails to take final action before the end of the ROP term, the existing ROP does not expire until the renewal is issued or denied, and the permit shield shall extend beyond the original ROP term until the department takes final action. **(R 336.1217(1)(c), R 336.1217(1)(a))**

## Revisions

1. For changes to any process or process equipment covered by this ROP that do not require a revision of the ROP pursuant to Rule 216, the permittee must comply with Rule 215. **(R 336.1215, R 336.1216)**
2. A change in ownership or operational control of a stationary source covered by this ROP shall be made pursuant to Rule 216(1). **(R 336.1219(2))**
3. For revisions to this ROP, an administratively complete application shall be considered timely if it is received by the department in accordance with the time frames specified in Rule 216. **(R 336.1210(10))**
4. Pursuant to Rule 216(1)(b)(iii), Rule 216(2)(d) and Rule 216(4)(d), after a change has been made, and until the department takes final action, the permittee shall comply with both the applicable requirements governing the change and the ROP terms and conditions proposed in the application for the modification. During this time period, the permittee may choose to not comply with the existing ROP terms and conditions that the application seeks to change. However, if the permittee fails to comply with the ROP terms and conditions proposed in the application during this time period, the terms and conditions in the ROP are enforceable. **(R 336.1216(1)(c)(iii), R 336.1216(2)(d), R 336.1216(4)(d))**

## Reopenings

1. A ROP shall be reopened by the department prior to the expiration date and revised by the department under any of the following circumstances:
	1. If additional requirements become applicable to this stationary source with three or more years remaining in the term of the ROP, but not if the effective date of the new applicable requirement is later than the ROP expiration date. **(R 336.1217(2)(a)(i))**
	2. If additional requirements pursuant to Title IV of the CAA become applicable to this stationary source. **(R 336.1217(2)(a)(ii))**
	3. If the department determines that the ROP contains a material mistake, information required by any applicable requirement was omitted, or inaccurate statements were made in establishing emission limits or the terms or conditions of the ROP. **(R 336.1217(2)(a)(iii))**
	4. If the department determines that the ROP must be revised to ensure compliance with the applicable requirements. **(R 336.1217(2)(a)(iv))**

## Renewals

1. For renewal of this ROP, an administratively complete application shall be considered timely if it is received by the department not more than 18 months, but not less than 6 months, before the expiration date of the ROP. **(R 336.1210(9))**

## Stratospheric Ozone Protection

1. If the permittee is subject to Title 40 of the Code of Federal Regulations (CFR), Part 82 and services, maintains, or repairs appliances except for motor vehicle air conditioners (MVAC), or disposes of appliances containing refrigerant, including MVAC and small appliances, or if the permittee is a refrigerant reclaimer, appliance owner or a manufacturer of appliances or recycling and recovery equipment, the permittee shall comply with all applicable standards for recycling and emissions reduction pursuant to 40 CFR Part 82, Subpart F.
2. If the permittee is subject to 40 CFR Part 82 and performs a service on motor (fleet) vehicles when this service involves refrigerant in the MVAC, the permittee is subject to all the applicable requirements as specified in 40 CFR Part 82, Subpart B, Servicing of Motor Vehicle Air Conditioners. The term “motor vehicle” as used in Subpart B does not include a vehicle in which final assembly of the vehicle has not been completed by the original equipment manufacturer. The term MVAC as used in Subpart B does not include the air-tight sealed refrigeration system used for refrigerated cargo or an air conditioning system on passenger buses using Hydrochlorofluorocarbon-22 refrigerant.

## Risk Management Plan

1. If subject to Section 112(r) of the CAA and 40 CFR Part 68, the permittee shall register and submit to the USEPA the required data related to the risk management plan for reducing the probability of accidental releases of any regulated substances listed pursuant to Section 112(r)(3) of the CAA as amended in 40 CFR 68.130. The list of substances, threshold quantities, and accident prevention regulations promulgated under 40 CFR Part 68, do not limit in any way the general duty provisions under Section 112(r)(1).
2. If subject to Section 112(r) of the CAA and 40 CFR Part 68, the permittee shall comply with the requirements of 40 CFR Part 68, no later than the latest of the following dates as provided in 40 CFR 68.10(a):
	1. June 21, 1999,
	2. Three years after the date on which a regulated substance is first listed under 40 CFR 68.130, or
	3. The date on which a regulated substance is first present above a threshold quantity in a process.
3. If subject to Section 112(r) of the CAA and 40 CFR Part 68, the permittee shall submit any additional relevant information requested by any regulatory agency necessary to ensure compliance with the requirements of 40 CFR Part 68.
4. If subject to Section 112(r) of the CAA and 40 CFR Part 68, the permittee shall annually certify compliance with all applicable requirements of Section 112(r) as detailed in Rule 213(4)(c)). **(40 CFR Part 68)**

## Emission Trading

1. Emission averaging and emission reduction credit trading are allowed pursuant to any applicable interstate or regional emission trading program that has been approved by the Administrator of the USEPA as a part of Michigan’s State Implementation Plan. Such activities must comply with Rule 215 and Rule 216. **(R 336.1213(12))**

## Permit to Install (PTI)

1. The process or process equipment included in this permit shall not be reconstructed, relocated, or modified unless a PTI authorizing such action is issued by the department, except to the extent such action is exempt from the PTI requirements by any applicable rule.2 **(R 336.1201(1))**
2. The department may, after notice and opportunity for a hearing, revoke PTI terms or conditions if evidence indicates the process or process equipment is not performing in accordance with the terms and conditions of the PTI or is violating the department’s rules or the CAA.2 **(R 336.1201(8), Section 5510 of Act 451)**
3. The terms and conditions of a PTI shall apply to any person or legal entity that now or hereafter owns or operates the process or process equipment at the location authorized by the PTI. If a new owner or operator submits a written request to the department pursuant to Rule 219 and the department approves the request, this PTI will be amended to reflect the change of ownership or operational control. The request must include all of the information required by Subrules (1)(a), (b) and (c) of Rule 219. The written request shall be sent to the appropriate AQD District Supervisor, EGLE.2**(R 336.1219)**
4. If the installation, reconstruction, relocation, or modification of the equipment for which PTI terms and conditions have been approved has not commenced within 18 months of the original PTI issuance date, or has been interrupted for 18 months, the applicable terms and conditions from that PTI, as incorporated into the ROP, shall become void unless otherwise authorized by the department. Furthermore, the person to whom that PTI was issued, or the designated authorized agent, shall notify the department via the Supervisor, Permit Section, EGLE, AQD, P. O. Box 30260, Lansing, Michigan 48909, if it is decided not to pursue the installation, reconstruction, relocation, or modification of the equipment allowed by the terms and conditions from that PTI.2 **(R 336.1201(4))**

**Footnotes:**

1This condition is state-only enforceable and was established pursuant to Rule 201(1)(b).

2This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

# B. SOURCE-WIDE CONDITIONS

Part B outlines the Source-Wide Terms and Conditions that apply to this stationary source. The permittee is subject to these special conditions for the stationary source in addition to the general conditions in Part A and any other terms and conditions contained in this ROP.

The permittee shall comply with all specific details in the special conditions and the underlying applicable requirements cited. If a specific condition type does not apply to this source, NA (not applicable) has been used in the table. If there are no Source-Wide Conditions, this section will be left blank.

# C. EMISSION UNIT SPECIAL CONDITIONS

Part C outlines terms and conditions that are specific to individual emission units listed in the Emission Unit Summary Table. The permittee is subject to the special conditions for each emission unit in addition to the General Conditions in Part A and any other terms and conditions contained in this ROP.

The permittee shall comply with all specific details in the special conditions and the underlying applicable requirements cited. If a specific condition type does not apply, NA (not applicable) has been used in the table. If there are no conditions specific to individual emission units, this section will be left blank.

## EMISSION UNIT SUMMARY TABLE

The descriptions provided below are for informational purposes and do not constitute enforceable conditions.

| **Emission Unit ID** | **Emission Unit Description****(Including Process Equipment & Control Device(s))** | **Installation****Date/****Modification Date** | **Flexible Group ID** |
| --- | --- | --- | --- |
| EUAUTODIP | Automatic dip system for applying cement to metal and plastic parts. Process also includes conveyor system for drying the dipped parts. The cements are dried by an electric dryer. VOC emissions from this line are controlled by a Regenerative Thermal Oxidizer. | 05-01-201305-04-2015 | FGAUTODIPFGRTOFGMACTMMMM |
| EUAUTODIP2 | Automatic dip system number 2 for applying cement to metal and plastic parts. Process also includes conveyor system for drying the dipped parts. The cements are dried by an electric dryer. VOC emissions from this line are controlled by a Regenerative Thermal Oxidizer. | 01-27-199807-13-201205-04-2015 | FGAUTODIPFGRTOFGMACTMMMM |
| EUCOE1 | Chain-on-edge number 1 is two automated booths for applying cement to metal and plastic parts. Prior to entering the booths, the parts first pass through a pre-heat oven. The chain-on-edge rotates the parts through the spray guns. VOC emissions from this line are controlled by a Regenerative Thermal Oxidizer. | 07-18-200507-13-201205-04-2015 | FGSPRAYMACHINESFGRTOFGMACTMMMM |
| EUCOE2 | Chain-on-edge number 2 is two automated booths for applying cement to metal and plastic parts. Prior to entering the booths, the parts first pass through a pre-heat oven. The chain-on-edge rotates the parts through the spray guns. VOC emissions from this line are controlled by a Regenerative Thermal Oxidizer. | 07-18-200507-13-201205-04-2015 | FGSPRAYMACHINESFGRTOFGMACTMMMM |
| EUCOE3 | Chain-on-edge number 3 is two automated booths for applying cement to metal and plastic parts. The chain-on-edge rotates the parts through the spray guns and then dries the parts in an oven. VOC emissions from this line are controlled by a Regenerative Thermal Oxidizer. | 01-01-198607-13-201205-04-2015 | FGSPRAYMACHINESFGRTOFGMACTMMMM |
| EUCOE4 | Chain-on-edge number 4 is two automated booths for applying cement to metal and plastic parts. Prior to entering the booths, the parts first pass through a pre- heat oven. The chain-on-edge rotates the parts through the spray guns. VOC emissions from this line are controlled by a common Regenerative Thermal Oxidizer. | 08-01-2015 | FGSPRAYMACHINESFGRTOFGMACTMMMM |
| EUROLLCOAT | A roll coat process with primer and adhesive application stations connected by a conveyor system. The cements are dried by an electric dryer. VOC emissions from the system are controlled by a Regenerative Thermal Oxidizer. | 05-20-2013 | FGRTOFGMACTMMMM |
| EUROTSPRAY1 | A rotary spray booth that applies adhesive to metal and plastic parts. The cements are dried by an electric dryer. VOC emissions from the system are controlled by a common Regenerative Thermal Oxidizer. | 11-21-2017 | FGSPRAYMACHINESFGRTOFGMACTMMMM |
| EURBRMOLDING | Rubber injection and compression presses. Emissions from presses and oven are controlled by fabric filters. | 05-01-196104-13-2016 | NA |
| EUSERVICE-BOOTH | Small services spray booth exempt under Rule 287(2)(c). Dry fabric filter controls. | 07-18-2005 | FGRULE287(2)(c) |
| EUCOLDCLEANER | Any cold cleaner that is grandfathered or exempt from Rule 201 pursuant to Rule 278 and Rule 281(2)(h) or Rule 285(2)(r)(iv). Existing cold cleaners were placed into operation prior to July 1, 1979. New cold cleaners were placed into operation on or after July 1, 1979. | 01-27-1998 | FGCOLDCLEANERS |
| EURBRCUREOVEN | A post-bond cure oven. Dry, cured rubber parts coming off the cementing lines are pushed into metal cans to form an assembly. An oil is used for lubrication to form the assembly and the parts are placed into the cure oven. Emissions are vented through dry fabric filters. | 10-1-2020 | NA |

## EUROLLCOAT

**EMISSION UNIT CONDITIONS**

**DESCRIPTION**

A roll coat process with primer and adhesive application stations connected by a conveyor system. The cements are dried by an electric dryer. VOC emissions from the system are controlled by a Regenerative Thermal Oxidizer.

**Flexible Group ID:** FGRTO, FGMACTMMMM

**POLLUTION CONTROL EQUIPMENT**

Dry Fabric Filters, Regenerative Thermal Oxidizer

**I. EMISSION LIMIT(S)**

NA

**II. MATERIAL LIMIT(S)**

NA

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall capture all waste cements, adhesives, coatings, thinners, additives and catalysts and shall store them in closed containers. The permittee shall dispose of all waste cements, adhesives, coatings, thinners, additives and catalysts in an acceptable manner in compliance with all applicable state rules and federal regulations.2 **(R 336.1224, R 336.1702(a))**
2. The permittee shall maintain a MAP for the equipment listed in this permit. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits. This MAP must address the startup, shutdown and corrective actions in the event of a malfunction of the emission capture system or the add-on control device. The MAP must also address any coating operation equipment that may cause increased emissions or that would affect capture efficiency if the process equipment malfunctions, such as conveyors that move parts among enclosures. **(R 336.1213(3), R 336.1910, R 336.1911)**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The permittee shall equip and maintain the application booth portions of EUROLLCOAT with non-atomizing applicators or comparable technology with equivalent transfer efficiency. For HVLP applicators, the permittee shall keep test caps available for pressure testing.2 **(R 336.1702(a))**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall install, calibrate, maintain and operate, in a satisfactory manner, a differential pressure gauge to monitor the pressure differential between the enclosure for EUROLLCOAT and the outside area on a continuous basis. The permittee shall keep, in a satisfactory manner, records of the pressure differential measurements. The measurements shall be recorded once per shift. The permittee shall keep all records on file and make them available to the Department upon request.2 **(R 336.1205, R 336.1224, R 336.1225,
R 336.1702)**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

The exhaust gases from the stacks listed in the table below shall be discharged unobstructed vertically upwards to the ambient air unless otherwise noted:

| **Stack & Vent ID** | **Maximum Exhaust Diameter / Dimensions****(inches)** | **Minimum Height Above Ground****(feet)** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- |
| 1. SVRTO
 | 302 | 422 | **R 336.1225****R 336.1901(a)****R 336.2803****R 336.2804****40 CFR 52.21(c)&(d)** |

**IX. OTHER REQUIREMENT(S)**

NA

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

## EURBRMOLDING

**EMISSION UNIT CONDITIONS**

**DESCRIPTION**

Rubber injection and compression presses. Emissions from presses and oven are controlled by fabric filters.

**Flexible Group ID:** NA

**POLLUTION CONTROL EQUIPMENT**

Dry Fabric Filters

**I. EMISSION LIMIT(S)**

| **Pollutant** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. VOCs
 | 7.8 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EURBRMOLDING | SC VI.3 SC VI.5 | **R 336.1702(a)** |
| 1. PM
 | 1.35 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EURBRMOLDING | SC VI.4 SC VI.5 | **R 336.1331** |
| 1. PM10
 | 1.35 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EURBRMOLDING | SC VI.4 SC VI.5 | **40 CFR 52.1(c)&(d)** |
| 1. PM2.5
 | 1.35 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EURBRMOLDING | SC VI.4 SC VI.5 | **40 CFR 52.1(c)&(d)** |

**II. MATERIAL LIMIT(S)**

1. The mold release agents used in EURBRMOLDING shall not contain any VOCs as defined by the supplier’s MSDS information.2 **(R 336.1702(a))**
2. The permittee shall not process more than 18,000,000 pounds of rubber in EURBRMOLDING per year based upon a 12-month rolling time period as determined at the end of each calendar month.2 **(R 336.1225,
R 336.1702(a), 40 CFR 52.1(c)&(d))**

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall not operate EURBRMOLDING unless the fabric filters are installed, maintained, and operated in a satisfactory manner, which includes following the maintenance and operating parameters specified in the MAP.2 **(R 336.1224, R 336.1225, R 336.1331, R 336.1910, 40 CFR 52.21(c)&(d))**
2. No later than 45 days after issuance of this permit, the permittee shall submit to the AQD District Supervisor, for review and approval, a MAP, as described in Rule 911(2), for EURBRMOLDING. After approval of the MAP by the AQD District Supervisor, the permittee shall not operate EURBRMOLDING unless the MAP, or an alternate plan approved by the AQD District Supervisor, is implemented and maintained. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits.2 **(R 336.1224,
R 336.1225, R 336.1331, R 336.1910, R 336.1911, 40 CFR 52.21(c) and (d))**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The permittee shall equip and maintain EURBRMOLDING with fabric filters.2 **(R 336.1224, R 336.1225,
R 336.1331, 40 CFR 52.21(c)&(d))**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall keep, in a satisfactory manner, records of the amount of each rubber molding material processed in EURBRMOLDING on a monthly and 12 month rolling time period basis, as determined at the end of each calendar month.2 **(R 336.1225, R 336.1331, R 336.1702(a), 40 CFR 52.21(c)&(d))**
2. The permittee shall maintain a current record of the chemical composition of each rubber molding material and mold release agent, including the weight percent of each component. The data may consist of MSDS, manufacturer’s formulation data, or both as deemed acceptable by the AQD District Supervisor.2 **(R 336.1224, R 336.1225, R 336.1702(a))**
3. The permittee shall keep, in a satisfactory manner, monthly and 12-month rolling time period VOC emission calculation records for EURBRMOLDING. Calculations shall be based on MSDS, manufacturer’s formulation data, and AP-42 emission factors or other source-specific emission factors, as deemed acceptable by the AQD District Supervisor.2 **(R 336.1702(a))**
4. The permittee shall keep, in a satisfactory manner, monthly and 12-month rolling time period PM, PM10, and PM2.5 emission calculation records for EURBRMOLDING. Calculations shall be based on the assumption that 0.05% (by weight) of the rubber used is emitted as PM, PM10, and PM2.5, and shall also take into account 70% control efficiency of the fabric filters. The permittee may use another method of calculation as deemed acceptable by the AQD District Supervisor.2 **(R 336.1331, 40 CFR 52.21 (c)&(d))**
5. The permittee shall keep records and calculations on file at the facility and make them available to the Department upon request. All required emissions calculations shall be completed by the 15th day of each the calendar month, for the previous month.2 **(R 336.1225, R 336.1331, R 336.1702(a), 40 CFR 52.21(c)&(d))**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

NA

**IX. OTHER REQUIREMENT(S)**

NA

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

## EURBRCUREOVEN

**EMISSION UNIT CONDITIONS**

**DESCRIPTION**

A post-bond cure oven. Dry, cured rubber parts coming off the cementing lines are pushed into metal cans to form an assembly. An oil is used for lubrication to form the assembly and the parts are placed into the cure oven. Emissions are vented through dry fabric filters.

**Flexible Group ID:** NA

**POLLUTION CONTROL EQUIPMENT**

Dry fabric filters

**I. EMISSION LIMIT(S)**

| **Pollutant** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. VOCs
 | 1.89 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EURBRCUREOVEN | SC VI.3 | **R 336.1702(a)** |

**II. MATERIAL LIMIT(S)**

| **Material** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. Post-bond oil
 | 3.44 lb / 8‑hours1 | 8-hour time period | EURBRCUREOVEN | SC VI.3 | **R 336.1225** |

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall capture all waste materials and shall store them in closed containers. The permittee shall dispose of all waste materials in an acceptable manner in compliance with all applicable state rules and federal regulations.2 **(R 336.1225, R 336.1702(a))**
2. The permittee shall dispose of spent filters in a manner which minimizes the introduction of air contaminants to the outer air.2 **(R 336.1370(1))**
3. The permittee shall maintain a MAP for the equipment listed in this permit. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits. This MAP must address the startup, shutdown and corrective actions in the event of a malfunction of the emission capture system or the add-on control device. The MAP must also address any coating operation equipment that may cause increased emissions or that would affect capture efficiency if the process equipment malfunctions, such as conveyors that move parts among enclosures. **(R 336.1213(3), R 336.1910, R 336.1911)**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The permittee shall not operate EURBRCUREOVEN unless all respective exhaust filters are installed, maintained and operated in a satisfactory manner.2 **(R 336.1301, R 336.1910)**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall complete all required calculations in a format acceptable to the AQD District Supervisor by the 15th day of the calendar month, for the previous calendar month, unless otherwise specified in any monitoring/recordkeeping special condition.2 **(R 336.1702)**
2. The permittee shall maintain a current listing from the manufacturer of the chemical composition of each material, including the weight percent of each component. The data may consist of MSDS, manufacturer's formulation data, or both as deemed acceptable by the AQD District Supervisor. The permittee shall keep all records on file and make them available to the Department upon request.2 **(R 336.1225, R 336.1702)**
3. The permittee shall keep the following information for EURBRCUREOVEN:
	1. Pounds of each material used, on both an 8-hour time period and on a monthly basis.
	2. VOC content (with water) of each material as applied.
	3. VOC mass emission calculations determining the monthly emission rate in tons per calendar month.
	4. VOC mass emission calculations determining the annual emission rate in tons per 12-month rolling time period as determined at the end of each calendar month.

The permittee shall keep the records using mass balance, or an alternative method and format acceptable to the AQD District Supervisor. The permittee shall keep all records on file and make them available to the Department upon request.2 **(R 336.1225, R 336.1702(a))**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

The exhaust gases from the stacks listed in the table below shall be discharged unobstructed vertically upwards to the ambient air unless otherwise noted:

| **Stack & Vent ID** | **Maximum Exhaust Diameter / Dimensions****(inches)** | **Minimum Height** **Above Ground****(feet)** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- |
| 1. SVPOSTCUREOVEN
 | 102 | 382 | **R 336.1225,****40 CFR 52.21(c)&(d)** |

**IX. OTHER REQUIREMENT(S)**

NA

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

# D. FLEXIBLE GROUP SPECIAL CONDITIONS

Part D outlines the terms and conditions that apply to more than one emission unit. The permittee is subject to the special conditions for each flexible group in addition to the General Conditions in Part A and any other terms and conditions contained in this ROP.

The permittee shall comply with all specific details in the special conditions and the underlying applicable requirements cited. If a specific condition type does not apply, NA (not applicable) has been used in the table. If there are no special conditions that apply to more than one emission unit, this section will be left blank.

## FLEXIBLE GROUP SUMMARY TABLE

The descriptions provided below are for informational purposes and do not constitute enforceable conditions.

| **Flexible Group ID** | **Flexible Group Description** | **Associated****Emission Unit IDs** |
| --- | --- | --- |
| FGAUTODIP | Two automatic dip systems for applying cement to metal and plastic parts. Processes also include conveyor systems for drying the dipped parts. The cements are dried by an electric dryer. VOC emissions from both lines are controlled by a Regenerative Thermal Oxidizer. | EUAUTODIPEUAUTODIP2 |
| FGSPRAYMACHINES | Chain-on-edge (COE) numbers 1, 2, and 4 consist of two automated booths each for applying cement to metal and plastic parts. Prior to entering the booths, the parts first pass through a pre- heat oven. COE number 3 is an automated booth for applying cement to metal and plastic parts; however, parts do not pass through a pre-heat oven. The chain-on-edge rotates the parts through the spray guns. VOC emissions from these lines are controlled by a common Regenerative Thermal Oxidizer.EUROTSPRAY1 is a rotary spray booth that applies adhesive to metal and plastic parts. The cements are dried by an electric dryer. VOC emissions from the system are controlled by a common Regenerative Thermal Oxidizer. | EUCOE1EUCOE2EUCOE3EUCOE4EUROTSPRAY1 |
| FGRTO | Two automatic dip spin lines, four automated chain-on-edge lines, a rotary spray line, and a roll coater all used to coat metal and plastic parts. The VOC emissions from these eight lines are controlled by a permanent total enclosure and common Regenerative Thermal Oxidizer. | EUAUTODIPEUAUTODIP2EUCOE1EUCOE2EUCOE3EUCOE4EUROLLCOATEUROTSPRAY1 |
| FGMACTMMMM | Each new, reconstructed, and existing affected source described in 40 CFR 63.3881(a)(1), including the subcategories listed in 40 CFR Part 63, Subpart MMMM, (40 CFR 63.3881(a)(2) through (6)), meeting the applicability requirements of 40 CFR 63.3881(b), which is engaged in the surface coating of miscellaneous metal parts and products. The affected source includes the collection of all the items listed in 40 CFR 63.3882(b)(1) through (4). Surface coating is defined by 40 CFR 63.3881 as the application of coating to a substrate using, for example, spray guns or dip tanks. Surface coating also includes associated activities, such as surface preparation, cleaning, mixing, and storage if they are directly related to the application of the coating. 40 CFR Part 63, Subpart MMMM does not apply to surface coating or a coating operation that meets any of the criteria of 40 CFR 63.3881(c)(1) through (17). | EUAUTODIPEUAUTODIP2EUCOE1EUCOE2EUCOE3EUCOE4EUROLLCOATEUROTSPRAY1 |
| FGRULE287(c) | Any emission unit that emits air contaminants and is exempt from the requirements of Rule 201 pursuant to Rule 278, Rule 278a and Rule 287(2)(c). Emission units installed / modified before December 20, 2016, may show compliance with Rule 287 in effect at the time of installation/modification. | EUSERVICE-BOOTH |
| FGCOLDCLEANERS | Any cold cleaner that is grandfathered or exempt from Rule 201 pursuant to Rule 278, Rule 278a and Rule 281(2)(h) or Rule 285(2)(r)(iv). Existing cold cleaners were placed into operation prior to July 1, 1979. New cold cleaners were placed into operation on or after July 1, 1979. | EUCOLDCLEANER |

## FGAUTODIP

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Two automatic dip systems for applying cement to metal and plastic parts. Processes also include conveyor systems for drying the dipped parts. The cements are dried by an electric dryer. VOC emissions from both lines are controlled by a Regenerative Thermal Oxidizer.

**Emission Units:** EUAUTODIP, EUAUTODIP2

**POLLUTION CONTROL EQUIPMENT**

Regenerative Thermal Oxidizer (RTO)

**I. EMISSION LIMIT(S)**

NA

**II. MATERIAL LIMIT(S)**

NA

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall capture all waste cements, adhesives, coatings, thinners, additives and catalysts and shall store them in closed containers. The permittee shall dispose of all waste cements, adhesives, coatings, thinners, additives and catalysts in an acceptable manner in compliance with all applicable state rules and federal regulations.2 **(R 336.1224, R 336.1702(a))**
2. The permittee shall maintain a MAP for the equipment listed in this permit. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits. This MAP must address the startup, shutdown and corrective actions in the event of a malfunction of the emission capture system or the add-on control device. The MAP must also address any coating operation equipment that may cause increased emissions or that would affect capture efficiency if the process equipment malfunctions, such as conveyors that move parts among enclosures. **(R 336.1213(3), R 336.1910, R 336.1911)**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

NA

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

The exhaust gases from the stacks listed in the table below shall be discharged unobstructed vertically upwards to the ambient air unless otherwise noted:

| **Stack & Vent ID** | **Maximum Exhaust Diameter / Dimensions****(inches)** | **Minimum Height Above Ground****(feet)** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- |
| 1. SVRTO
 | 302 | 422 | **R 336.1225****40 CFR 52.21(c)&(d)** |

**IX. OTHER REQUIREMENT(S)**

NA

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

## FGSPRAYMACHINES

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Chain-on-edge (COE) numbers 1, 2, and4 consist of two automated booths each for applying cement to metal and plastic parts. Prior to entering the booths, the parts first pass through a pre- heat oven. COE number 3 is an automated booth for applying cement to metal and plastic parts; however, parts do not pass through a pre-heat oven. The chain-on-edge rotates the parts through the spray guns. VOC emissions from these lines are controlled by a common Regenerative Thermal Oxidizer.

EUROTSPRAY1 is a rotary spray booth that applies adhesive to metal and plastic parts. The cements are dried by an electric dryer. VOC emissions from the system are controlled by a common Regenerative Thermal Oxidizer.

**Emission Units:** EUCOE1, EUCOE2, EUCOE3, EUCOE4, EUROTSPRAY1

**POLLUTION CONTROL EQUIPMENT**

Dry fabric filters, Regenerative Thermal Oxidizer (RTO)

**I. EMISSION LIMIT(S)**

NA

**II. MATERIAL LIMIT(S)**

NA

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall capture all waste cements, adhesives, coatings, thinners, additives and catalysts and shall store them in closed containers. The permittee shall dispose of all waste cements, adhesives, coatings, thinners, additives and catalysts in an acceptable manner in compliance with all applicable state rules and federal regulations.2 **(R 336.1224, R 336.1702(a))**
2. The permittee shall dispose of spent filters in a manner which minimizes the introduction of air contaminants to the outer air.2 **(R 336.1224, R 336.1370)**
3. The permittee shall maintain a MAP for the equipment listed in this permit. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits. This MAP must address the startup, shutdown and corrective actions in the event of a malfunction of the emission capture system or the add-on control device. The MAP must also address any coating operation equipment that may cause increased emissions or that would affect capture efficiency if the process equipment malfunctions, such as conveyors that move parts among enclosures. **(R 336.1213(3), R 336.1910, R 336.1911)**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The permittee shall not operate the spray booth portions of FGSPRAYMACHINES unless all respective exhaust filters are installed, maintained, and operated in a satisfactory manner.2 **(R 336.1224, R 336.1910)**
2. The permittee shall equip and maintain the spray booth portions of FGSPRAYMACHINES with HVLP applicators or comparable technology with equivalent transfer efficiency. For HVLP applicators, the permittee shall keep test caps available for pressure testing.2 **(R 336.1702(a))**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

1. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**VIII. STACK/VENT RESTRICTION(S)**

The exhaust gases from the stacks listed in the table below shall be discharged unobstructed vertically upwards to the ambient air unless otherwise noted:

| **Stack & Vent ID** | **Maximum Exhaust Diameter / Dimensions****(inches)** | **Minimum Height Above Ground****(feet)** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- |
| 1. SVRTO
 | 302 | 422 | **R 336.1225,****40 CFR 52.21(c)&(d)** |

**IX. OTHER REQUIREMENT(S)**

NA

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

## FGRTO

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Two automatic dip spin lines, four automated chain-on-edge lines, a rotary spray line, and a roll coater all used to coat metal and plastic parts. The VOC emissions from these eight lines are controlled by a permanent total enclosure and common Regenerative Thermal Oxidizer.

**Emission Units:** EUAUTODIP, EUAUTODIP2, EUCOE1, EUCOE2, EUCOE3, EUCOE4, EUROLLCOAT, and EUROTSPRAY1

**POLLUTION CONTROL EQUIPMENT**

Permanent Total Enclosure (PTE) on each coating booth, and Regenerative Thermal Oxidizer (RTO)

**I. EMISSION LIMIT(S)**

| **Pollutant** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. VOCs
 | 56.4 tpy2 | 12-month rolling time period as determined at the end of each calendar month | FGRTO | SC VI.2SC VI.3 | **R 336.1205, R 336.1702(a)** |
| 1. VOCs
 | 4.8 tpy2 | 12-month rolling time period as determined at the end of each calendar month | EUROTSPRAY1 | SC VI.2SC VI.3 | **R 336.1702(a)** |
| 1. Ethylbenzene (CAS #100-41-4)
 | 10.0 tpy1 | 12-month rolling time period as determined at the end of each calendar month | FGRTO | SC VI.2SC VI.4 | **R 336.1225** |

**II. MATERIAL LIMIT(S)**

NA

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. The permittee shall not operate FGRTO unless a malfunction abatement plan (MAP) as described in Rule 911(2) is implemented and maintained. The MAP shall, at a minimum, specify the following:
	1. A complete preventative maintenance program including identification of the supervisory personnel responsible for overseeing the inspection, maintenance, and repair of air-cleaning devices, a description of the items or conditions that shall be inspected, the frequency of the inspections or repairs, and an identification of the major replacement parts that shall be maintained in inventory for quick replacement.
	2. An identification of the source and air-cleaning device operating variables that shall be monitored to detect a malfunction or failure, the normal operating range of these variables, and a description of the method of monitoring or surveillance procedures.
	3. A description of the corrective procedures or operational changes that shall be taken in the event of a malfunction or failure to achieve compliance with the applicable emission limits.

If at any time the MAP fails to address or inadequately addresses an event that meets the characteristics of a malfunction, the permittee shall amend the MAP within 45 days after such an event occurs. The permittee shall also amend the MAP within 45 days, if new equipment is installed or upon request from the District Supervisor. The permittee shall submit the MAP and any amendments to the MAP to the AQD District Supervisor for review and approval. If the AQD does not notify the permittee within 90 days of submittal, the MAP or amended MAP shall be considered approved. Until an amended plan is approved, the permittee shall implement corrective procedures or operational changes to achieve compliance with all applicable emission limits.2 **(R 336.1225,
R 336.1702(a), R 336.1910, R 336.1911, 40 CFR 52.21(c) and (d))**

1. The permittee shall maintain a minimum of 0.007 inches of water pressure differential between the PTE and the adjacent area on a continuous basis.2 **(R 336.1205, R 336.1702(a))**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The permittee shall not operate FGRTO unless the RTO is installed, maintained and operated in a satisfactory manner. Satisfactory operation of the RTO includes a minimum VOC destruction efficiency of 95% (by weight), maintaining a minimum temperature of 1,500°F, and a minimum retention time of 0.5 seconds. The minimum temperature may be adjusted based on the most recent acceptable stack test which achieved a minimum overall destruction efficiency of 95%.2 **(R 336.1205, R 336.1225, R 336.1702, R 336.1910)**
2. The permittee shall not operate any spray booth portion in FGRTO unless their respective PTE is installed, maintained and operated in a satisfactory manner. Satisfactory operation requires that each PTE is operating at a pressure lower than all respective adjacent areas so that air flows into each PTE through all Natural Draft Openings. Natural Draft Opening is defined as any opening that is not connected to a duct in which a fan or blower is installed.2 **(R 336.1205, R 336.1702(a), R 336.1910)**
3. The permittee shall install, calibrate, maintain and operate in a satisfactory manner a temperature monitoring device in the combustion chamber of the RTO to monitor the temperature on a continuous basis during operation of FGRTO.2 **(R 336.1224, R 336.1225, R 336.1702)**
4. The permittee shall install, calibrate, maintain and operate, in a satisfactory manner, a differential pressure gauge to monitor the pressure differential between each PTE in FGRTO and the respective outside area on a continuous basis during operation of the respective portion of FGRTO.2 **(R 336.1205, R 336.1702(a), R 336.1910)**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The VOC content, water content and density of any adhesives and coatings, as applied and as received, shall be determined randomly on a yearly basis with all coatings and adhesives tested within a five-year period using federal Reference Test Method 24. Upon prior approval by the AQD District Supervisor, the VOC content may be determined from manufacturer’s formulation data. If the Method 24 and the formulation values should differ, then the Method 24 results shall be used to determine compliance.2 **(R 336.1702(a))**
2. The permittee shall verify destruction efficiency of the RTO by testing at the owner’s expense, in accordance with the Department requirements. Testing shall be performed using an approved USEPA Method listed in
40 CFR Part 60, Appendix A. An alternate method, or a modification to the approved USEPA Method, may be specified in an AQD approved Test Protocol. No less than 30 days prior to testing, the permittee shall submit a complete test plan to the AQD Technical Programs Unit and District Office. The AQD must approve the final plan prior to testing, including any modifications to the method in the test protocol that are proposed after initial submittal. The permittee must submit a complete report of the test results to the AQD Technical Programs Unit and District Office within 60 days following the last date of the test.2 **(R 336.2001, R 336.2003, R 336.2004,
R 336.1205, R 336.1224, R 336.1225, R 336.1702, 40 CFR 52.21(c)&(d))**
3. Testing must meet the requirements of the federal Clean Air Act, all applicable state and federal rules and regulations, and be within the authority of the AQD to make the change. **(R 336.1213(3))**
4. The permittee shall verify destruction efficiency of the RTO by testing, at a minimum, every five years from the date of the last test. **(R 336.1213(3), R 336.2001, R 336.2003, R 336.2004)**
5. The permittee shall notify the AQD Technical Programs Unit Supervisor and the District Supervisor not less than 7 days before testing of the time and place performance tests will be conducted. **(R 336.1213(3),
R 336.2001(4))**

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall complete all required calculations in a format acceptable to the AQD District Supervisor by the 15th day of the calendar month, for the previous calendar month, unless otherwise specified in any monitoring/recordkeeping special condition.2 **(R 336.1205, R 336.1225, R 336.1702)**
2. The permittee shall maintain a current listing from the manufacturer of the chemical composition of each cement, adhesive, coating, thinner, solvent, additive, and catalyst, including the weight percent of each component. The data may consist of MSDS, manufacturer’s formulation data, or both as deemed acceptable by the AQD District Supervisor. The permittee shall keep all records on file and make them available to the Department upon request.2 **(R 336.1225, R 336.1702)**
3. The permittee shall keep the following information on a monthly basis for EUROTSPRAY1 and FGRTO:
	1. Gallons (with water) of each material used and, if applicable, reclaimed.
	2. VOC content (with water) of each material as applied.
	3. VOC mass emission calculations determining the monthly emission rate in tons per calendar month.
	4. VOC mass emission calculations determining the annual emission rate in tons per 12-month rolling time period as determined at the end of each calendar month.

The permittee shall keep the records using mass balance or an alternate method and format acceptable to the AQD District Supervisor. The permittee shall keep all records on file and make them available to the Department upon request.2 **(R 336.1205, R 336.1225, R 336.1702)**

1. The permittee shall keep the following information on a monthly basis for FGRTO:
	1. Gallons (with water) of each ethylbenzene containing material used and, if applicable, reclaimed.
	2. The ethylbenzene content (with water) in pounds per gallon of each material used.
	3. Ethylbenzene mass emission calculations determining the monthly emission rate in tons per calendar month.
	4. Ethylbenzene mass emission calculations determining the annual emission rate in tons per 12-month rolling time period as determined at the end of each calendar month.

The permittee shall keep the records using mass balance or an alternate method and format acceptable to the AQD District Supervisor. The permittee shall keep all records on file and make them available to the Department upon request.1 **(R 336.1225)**

1. The permittee shall monitor and record, in a satisfactory manner, the temperature in the combustion chamber of the RTO on a continuous basis, during operation of FGRTO. Temperature data recording shall consist of measurements made at equally spaced intervals, not to exceed 15 minutes per interval. All records shall be kept on file and made available to the Department upon request.2 **(R 336.1702)**
2. The permittee shall monitor and record, in a satisfactory manner, the pressure differential between each PTE for FGRTO and the outside area, on a continuous basis, to verify that air is entering each of the PTE. The permittee shall keep all records on file and make them available to the Department upon request.2
**(R 336.1205, R 336.1702)**
3. The permittee shall continuously monitor and record the combustion chamber temperature of the RTO, as described in SC VI.5 (above) as an indicator of proper operation of the RTO. The indicator range is a minimum combustion temperature of 1500°F during operation of the RTO. An excursion is defined as a 3-hour block average temperature that is less than the required minimum temperature of 1500°F. The monitor shall be calibrated or replaced annually. **(40 CFR 64.6(c)(1)(i), (ii), & (iii), 40 CFR 64.6(c)(2))**
4. The permittee shall evaluate the capture efficiency of the capture system by monitoring the differential pressure across each enclosure. This shall be monitored and recorded as described in SC VI.6 (above) on a data acquisition system or other method or manually logged once per day. The indicator range is a minimum pressure drop across each enclosure of at least 0.007 inches of water. An excursion is defined as a pressure drop reading less than 0.007 inches of water across an enclosure while equipment is in operation. The pressure gauge shall continuously monitor the pressure drop across the permanent total enclosures. Continuous monitoring is at least one reading every 15 minutes. The averaging period is instantaneous. The monitor shall be calibrated or replaced annually. **(40 CFR 64.3(a)(2), 40 CFR 64.6(c)(2), 40 CFR 64.6(c)(1)(iii))**
5. Upon detecting an excursion or exceedance, the owner or operator shall restore operation of the pollutant-specific emissions unit (including the control device and associated capture system) to its normal or usual manner of operation as expeditiously as practicable in accordance with good air pollution control practices for minimizing emissions. The response shall include minimizing the period of any startup, shutdown or malfunction and taking any necessary corrective actions to restore normal operation and prevent the likely recurrence of the cause of an excursion or exceedance (other than those caused by excused startup or shutdown conditions).

Corrective actions shall include:

RTO Combustion temperature: Follow corrective action included in the approved MAP; Logging and Reporting in Semi-Annual Reports.

Pressure drop across PTE: Interlocks will shut down the operation of the machine after 5 minutes of readings less than required minimum; Followed Logging and Reporting in a Semi-Annual Report are required if interlocks fail. **(40 CFR 64.7(d))**

1. Except for, as applicable, monitoring malfunctions, associated repairs, and required quality assurance or control activities (including, as applicable, calibration checks and required zero and span adjustments), the owner or operator shall conduct all monitoring in continuous operation (or shall collect data at all required intervals) at all times that the pollutant-specific emissions unit is operating. Data recorded during monitoring malfunctions, associated repairs, and required quality assurance or control activities shall not be used for purposes of this part, including data averages and calculations or fulfilling a minimum data availability requirement, if applicable. The owner or operator shall use all the data collected during all other periods in assessing the operation of the control device and associated control system. A monitoring malfunction is any sudden, infrequent, not reasonably preventable failure of the monitoring to provide valid data. Monitoring failures that are caused in part by poor maintenance or careless operation are not malfunctions. **(40 CFR 64.6(c)(3), 40 CFR 64.7(c))**
2. The permittee shall properly maintain the monitoring system, including keeping necessary parts for routine repair of the monitoring equipment. **(40 CFR 64.7(b))**
3. The permittee shall maintain records of monitoring data, monitor performance data, corrective actions taken, any written quality improvement plan and any activities undertaken to implement a quality improvement plan, and other information such as data used to document the adequacy of monitoring, or records of monitoring maintenance or corrective actions. **(40 CFR 64.9(b)(1))**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**
2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**
3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year.
**(R 336.1213(4)(c))**
4. The permittee shall submit any performance test reports to the AQD Technical Programs Unit and District Office, in a format approved by the AQD. **(R 336.1213(3)(c), R 336.2001(5))**
5. Each semiannual report of monitoring and deviations shall include summary information on the number, duration and cause of excursions and/or exceedances and the corrective actions taken. If there were no excursions and/or exceedances in the reporting period, then this report shall include a statement that there were no excursions and/or exceedances. **(40 CFR 64.9(a)(2)(i))**
6. Each semiannual report of monitoring and deviations shall include summary information on monitor downtime. If there were no periods of monitor downtime in the reporting period, then this report shall include a statement that there were no periods of monitor downtime. **(40 CFR 64.9(a)(2)(ii))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

The exhaust gases from the stacks listed in the table below shall be discharged unobstructed vertically upwards to the ambient air unless otherwise noted:

| **Stack & Vent ID** | **Maximum Exhaust Diameter / Dimensions****(inches)** | **Minimum Height Above Ground****(feet)** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- |
| 1. SVRTO
 | 302 | 422 | **R 336.1225****40 CFR 52.21(c)&(d)** |

**IX. OTHER REQUIREMENT(S)**

1. The permittee shall comply with all applicable requirements of 40 CFR Part 64. **(40 CFR Part 64)**
2. If the permittee identifies a failure to achieve compliance with an emission limitation or standard for which the approved monitoring did not provide an indication of an excursion or exceedance while providing valid data, or the results of compliance or performance testing document a need to modify the existing indicator ranges or designated conditions, the permittee shall promptly notify the AQD and if necessary, submit a proposed modification of the ROP and CAM Plan to address the necessary monitoring changes. Such a modification may include but is not limited to, reestablishing indicator ranges or designated conditions, modifying the frequency of conducting monitoring and collecting data, or the monitoring of additional parameters. **(40 CFR 64.7(e))**

**Footnotes:**

1 This condition is state only enforceable and was established pursuant to Rule 201(1)(b).

2 This condition is federally enforceable and was established pursuant to Rule 201(1)(a).

## FGMACTMMMM

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Each existing affected source described in 40 CFR 63.3881(a)(1), including the subcategories listed in 40 CFR
Part 63, Subpart MMMM,40 CFR63.3881(a)(2) through (6), meeting the applicability requirements of 40 CFR 63.3881(b), which is engaged in the surface coating of miscellaneous metal parts and products. The affected source includes the collection of all the items listed in 40 CFR 63.3882(b)(1) through (4). Surface coating is defined by 40 CFR 63.3881 as the application of coating to a substrate using, for example, spray guns or dip tanks. Surface coating also includes associated activities, such as surface preparation, cleaning, mixing, and storage if they are directly related to the application of the coating.

**Emission Units:** EUAUTODIP, EUAUTODIP2, EUCOE1, EUCOE2, EUCOE3, EUCOE4, EUROLLCOAT, and EUROTSPRAY1

**POLLUTION CONTROL EQUIPMENT**

Permanent Total Enclosure (PTE) on each coating booth, and Regenerative Thermal Oxidizer (RTO)

**I. EMISSION LIMIT(S)**

| **Pollutant** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. Organic HAP
 | 2.6 lbs pergal of coating solids2 | 12-month rolling time period as determined at the end of each month | Existing –General Use Coating | SC V.1,SC VI.1 through SC VI.8 | **40 CFR 63.3890(b)(1)** |
| 1. Organic HAP
 | 37.7 lbs per gal of coating solids2 | 12-month rolling time period as determined at the end of each month | Existing –Rubber-to-Metal Coating | SC V.1,SC VI.1 through SC VI.8 | **40 CFR 63.3890(b)(4)** |

1. The permittee shall determine whether the organic HAP emission rate is equal to or less than the applicable emission limits in 40 CFR 63.3890 using at least one of the following three options, which are listed in 40 CFR 63.3891(a) through (c):

a. Compliant material option,

b. Emission rate without add-on controls option, or

c. Emission rate with add-on controls option.

The permittee shall include all coatings, thinners, and/or other additives, and cleaning materials used when determining the emission rate. **(40 CFR 63.3891)**

1. Any coating operation(s) using the compliant material option or the emission rate without add-on controls option, shall be in compliance with the applicable emission limits in 40 CFR 63.3890 at all times. **(40 CFR 63.3900(a)(1))**
2. If the surface coating operation(s) meet the applicability criteria of more than one of the subcategory emission limits specified in 40 CFR 63.3890(a) or (b), the permittee may comply separately with each subcategory emission limit or comply using one of the alternatives in 40 CFR 63.3890(c)(1) or (2). **(40 CFR 63.3890(c))**
3. The permittee may comply with a facility-specific emission limit calculated from the relative amount of coating activity that is subject to each emission limit. If the permittee elects to comply using the facility-specific emission limit alternative, then compliance with the facility-specific emission limit and the emission limitations in this subpart for all surface coating operations constitutes compliance with this and other applicable surface coating NESHAP. The procedures for calculating the facility-specific emission limit are specified in 40 CFR 63.3890. In calculating a facility-specific emission limit, include coating activities that meet the applicability criteria of other surface coating NESHAP and constitute more than 1 percent of total coating activities at the facility. **(40 CFR 63.3881(e)(3))**

**II. MATERIAL LIMIT(S)**

For the compliant materials option, the permittee shall meet the material limits specified in the following table.

| **Material** | **Limit** | **Time Period/ Operating Scenario** | **Equipment** | **Monitoring/****Testing Method** | **Underlying Applicable Requirements** |
| --- | --- | --- | --- | --- | --- |
| 1. Each Thinner and/or Additive | No Organic HAP \* | Continuous | Each Coating Operation usingCompliant Material Option | SC VI.1SC VI.2SC VI.3SC VI.5 | **40 CFR 63.3891(a)** |
| 2. Each Cleaning Material | No Organic HAP \* | Continuous | Each Coating Operation usingCompliant Material Option | SC VI.1SC VI.2SC VI.3SC VI.5 | **40 CFR 63.3891(a)** |

\* Determined according to 40 CFR 63.3941(a).

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. At all times, the permittee must operate and maintain any affected source, including associated air pollution control equipment and monitoring equipment, in a manner consistent with safety and good air pollution control practices for minimizing emissions. **(40 CFR 63.3893)**

2. For any coating operation(s) using the emission rate with add-on controls option, the permittee must develop and implement a work practice plan, to minimize the organic HAP emissions from the storage, mixing and conveying of coatings, thinners and/or other additives, and cleaning materials used in, and waste materials generated by the controlled coating operation(s). The work practice plan must specifiy practices and procedures to ensure, at a minimum, the following elements are implemented:

a. All organic HAP containing coatings, thinners and/or other additives, cleaning materials, and waste materials must be stored in closed containers. **(40 CFR 63.3893(b)(1))**

b. Spills of organic HAP containing coatings, thinners and/or other additives, cleaning materials, and waste materials must be minimized. **(40 CFR 63.3893(b)(2))**

c. Organic HAP containing coatings, thinners and/or other additives, cleaning materials, and waste materials must be conveyed from one location to another in closed containers or pipes. **(40 CFR 63.3893(b)(3))**

d. Mixing vessels which contain organic-HAP-containing coatings and other materials must be closed except when adding to, removing, or mixing the contents. **(40 CFR 63.3893(b)(4))**

e. Emissions of organic HAP must be minimized during cleaning of storage, mixing, and conveying equipment. **(40 CFR 63.3893(b)(5))**

1. The coating operation(s) must be in compliance with the operating limits for emission capture systems and add-on control devices required by 40 CFR 63.3892 at all times, except for solvent recovery systems which conduct liquid-liquid material balances according to 40 CFR 63.3961(j). **(40 CFR 63.3900(a)(2)(ii))**
2. Any coating operation(s) using the emission rate with add-on controls option must be in compliance with the work practice standards in 40 CFR 63.3893 at all times. **(40 CFR 63.3900(a)(2)(iii))**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. For any coating operation(s) using the emission rate with add-on controls option, the permittee shall meet the operating limits specified in Table 1 of 40 CFR Part 63, Subpart MMMM as identified below. The permittee must establish the operating limits during the performance test according to the requirements in 40 CFR 63.3967. The permittee must meet the operating limits at all times after established. **(40 CFR 63.3892(b), 40 CFR Part 63, Subpart MMMM,** **Table 1)**

| **Add-on Control Device** | **Operating Limit** |
| --- | --- |
| Thermal oxidizer | The average combustion temperature in any 3-hour period must not fall below the combustion temperature limit established according to 40 CFR 63.3967(a).  |

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall determine the mass fraction of organic HAP for each material used, the mass fraction of coating solids for each coating, and the density of each material used in accordance with 40 CFR 63.3941, 40 CFR 63.3951, and/or 40 CFR 63.3961. **(40 CFR 63.3941, 40 CFR 63.3951, 40 CFR 63.3961)**
2. For any coating operation(s) using the emission rate with add-on controls option, the permittee must conduct each performance test required by 40 CFR 63.3960 according to the requirements in 40 CFR 63.3964(a)(1) and (2). The permittee must conduct each performance test of an emission capture system according to the requirements in 40 CFR 63.3965. The permittee must conduct each performance test of an add-on control device according to the requirements in 40 CFR 63.3966. No less than 30 days prior to testing, the permittee shall submit a complete test plan to the AQD Technical Programs Unit and District Office. The AQD must approve the final plan prior to testing. The permittee must submit a complete report of the test results to the AQD Technical Programs Unit and District Office within 60 days following the last date of the test. **(R 336.1213(3), R 336.2001, R 336.2002, R 336.2003, 40 CFR 63.3964(a) and (b))**

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall conduct an initial compliance demonstration for the initial compliance period according to the requirements in 40 CFR 63.3941, 40 CFR 63.3951, or 40 CFR 63.3961. The initial compliance period begins on the applicable compliance date specified in 40 CFR 63.3883 and ends on the last day of the 12th month following the compliance date. If the compliance date occurs on any day other than the first of the month, then the compliance period extends through that month plus the next 12 months. **(40 CFR 63.3940, 40 CFR 63.3950, 40 CFR 63.3960)**

2. The permittee shall keep all records required by 40 CFR 63.3930 in the format and timeframes outlined in 40 CFR 63.3931. **(40 CFR 63.3942(d), 40 CFR 63.3952(d), 40 CFR 63.3963(j))**

3. The permittee shall maintain, at a minimum, the following records for each compliance period:

a. A copy of each notification and report that is submitted to comply with Subpart MMMM, and the documentation supporting each notification and report. **(40 CFR 63.3930(a))**

b. A current copy of information provided by materials suppliers or manufacturers, such as manufacturer’s formulation data, or test data used to determine the mass fraction of organic HAP and density of each coating, thinner and/or other additive, and cleaning material, and the volume fraction of coating solids for each coating. **(40 CFR 63.3930(b))**

c. A list of the coating operations on which each compliance option was used, and the beginning and ending dates and times for each compliance option used. **(40 CFR 63.3930(c)(1))**

d. For the compliant materials option, the calculation of the organic HAP content for each coating, using Equation 2 of 40 CFR 63.3941. **(40 CFR 63.3930(c)(2))**

e. For the emission rate without add-on controls option, the calculation of the total mass of organic HAP emissions for the coatings, thinners and/or additives, and cleaning materials used each month using Equations 1, 1A through 1C and 2 of 40 CFR 63.3951; and, if applicable, the calculation used to determine mass of organic HAP in waste materials according to 40 CFR 63.3951(e)(4); the calculation of the total volume of coating solids used each month using Equation 2 of 40 CFR 63.3951; and the calculation of each 12-month organic HAP emission rate using Equation 3 of 40 CFR 63.3951. **(40 CFR 63.3930(c)(3))**

f. For the emission rate with add-on controls option, the calculations specified in 40 CFR 63.3930(c)(4)(i) through (v). **(40 CFR 63.3930(c)(4))**

g. The name and mass or volume of each coating, thinner and/or other additive, and cleaning material used during each compliance period. If the compliant material option is used for all coatings at the affected source, the permittee may maintain purchase records for each material used rather than a record of the volume used. **(40 CFR 63.3930(d))**

h. The mass fraction of organic HAP for each coating, thinner and/or additive, and cleaning material used during each compliance period unless the material is tracked by weight. **(40 CFR 63.3930(e))**

i. The volume fraction of coating solids for each coating used during each compliance period. **(40 CFR 63.3930(f))**

j. For either the emission rate without add-on controls or with add-on controls option, the density of for each coating, thinner and/or other additive, and cleaning material used during each compliance period. **(40 CFR 63.3930(g))**

k. The information specified in 40 CFR 63.3930(h)(1) through (3), if an allowance is used in Equation 1 of 40 CFR 63.3951 for organic HAP contained in waste materials sent to or designated for shipment to a treatment, storage, and disposal facility (TSDF) according to 40 CFR 63.3951(e)(4). **(40 CFR 63.3930(h))**

l. The date, time, and duration of each deviation. **(40 CFR 63.3930(j))**

m. For the emission rate with add-on controls option, records specified in 40 CFR 63.3930(k)(1) through 40 CFR 63.3930(k)(8). **(40 CFR 63.3930(k))**

4. For any coating operation(s) using the emission rate with add-on controls option, the permittee shall demonstrate continuous compliance with the operating limits specified in Table 1 of 40 CFR Part 63, Subpart MMMM using the applicable method(s) described below: **(40 CFR 63.3963(c))**

| **Add-on Control Device** | **Operating Limit** | **Continuous Compliance****Demonstration Method** |
| --- | --- | --- |
| Thermal oxidizer | 1. The average combustion temperature in any 3-hour period must not fall below the combustion temperature limit established according to 40 CFR 63.3967(a).
 | 1. Collect the combustion temperature data according to 40 CFR 63.3968(c)
2. Reduce the data to 3-hour block averages; and
3. Maintain the 3-hour average combustion temperature at or above the temperature limit.
 |

1. For each coating used for the compliant coating option, the permittee shall demonstrate continuous compliance with the emission limit in 40 CFR 63.3890, for each compliance period, using Equation 2 of 40 CFR 63.3941. For each thinner and cleaning material used, the permittee shall determine continuous compliance according to 40 CFR 63.3941(a). **(40 CFR 63.3942)**
2. For any coating operation or group of coating operations using the emission rate without add-on controls option, the permittee shall demonstrate continuous compliance with the applicable organic HAP emission limit in 40 CFR 63.3890, for each compliance period, according to 40 CFR 63.3951(a) through (g). **(40 CFR 63.3952)**
3. For any coating operation(s) using the emission rate with add-on controls option, the permittee shall demonstrate continuous compliance with the applicable organic HAP emission limit in 40 CFR 63.3890, for each compliance period, according to the procedures in 40 CFR 63.3961. **(40 CFR 63.3963)**
4. During the performance test required by 40 CFR 63.3960, the permittee shall perform the applicable monitoring and recordkeeping in accordance with 40 CFR 63.3967 to establish the emission capture system and add-on control device operating limits required by 40 CFR 63.3892. **(40 CFR 63.3967)**
5. For any coating operation(s) using the emission rate with add-on controls option, the permittee shall install, operate, and maintain each Continuous Parameter Monitoring System (CPMS) according to the requirements of 40 CFR 63.3968(a). If the capture system contains a bypass line, the permittee shall comply with the requirements of 40 CFR 63.3968(b). **(40 CFR 63.3968)**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked orreceived by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

1. For the compliant material option, the permittee shall report a deviation, as specified in 40 CFR 63.3910(c)(6) and 40 CFR 63.3920(a)(5), if any coating used for any 12-month compliance period exceeds the applicable emission limit specified in 40 CFR 63.3890; or any thinner or cleaning material used contains any organic HAP. **(40 CFR 63.3942(b))**

5. For the emission rate without add-on controls, the permittee shall report a deviation, as specified in 40 CFR 63.3910(c)(6) and 40 CFR 63.3920(a)(6), if the organic HAP emission rate for any 12-month compliance period exceeds the applicable emission limit specified in 40 CFR 63.3890. **(40 CFR 63.3952(b))**

6. For the emission rate with add-on controls option, the permittee shall report the following as deviations as specified in 40 CFR 63.3910(c)(6) and 40 CFR 63.3920(a)(7):

a. The organic HAP emission rate for any 12-month compliance period exceeds the applicable emission limit specified in 40 CFR 63.3890; **(40 CFR 63.3963(b))**

b. An operating parameter is out of the allowed range; **(40 CFR 63.3963(c)(1))**

c. Any control system by-pass line, for which liquid-liquid material balances are not carried out, is opened; **(40 CFR 63.3963(d))**

d. Deviations from work practice standards occur. **(40 CFR 63.3963(e))**

7. The permittee shall submit the applicable notifications specified in 40 CFR 63.7(b) and (c), 40 CFR 63.8(f)(4), 40 CFR 63.9(b) through (e) and (h), and an initial notification and a notification of compliance status as specified in 40 CFR 63.3910. **(40 CFR 63.3910)**

8. The permittee shall submit all semiannual compliance reports specified in 40 CFR 63.3920(a). Each semiannual compliance report shall identify which coating operation(s) used each compliance option, and if there were no deviations from the emission limitations in 40 CFR 63.3890, include a statement that the coating operations were in compliance. **(40 CFR 63.3920, 40 CFR 63.3942(c), 40 CFR 63.3952(c), 40 CFR 63.3963(f))**

1. The permittee must submit the following:
2. Within 60 days after the date of completing each performance test for emission capture systems and add-on control devices, the results of the performance tests required by 40 CFR Part 63, Subpart MMMM to the USEPA via the Compliance and Emissions Data Reporting Interface (CEDRI). The CEDRI interface can be accessed through the EPA's Central Data Exchange (CDX) ([*https://cdx.epa.gov/*](https://cdx.epa.gov/)). Performance test data must be submitted in the file format generated through use of the USEPA's Electronic Reporting Tool (ERT) (see [https://www.epa.gov/electronic-reporting-air-emissions/electronic-reporting-tool-ert](https://gcc02.safelinks.protection.outlook.com/?url=https%3A%2F%2Fwww.epa.gov%2Felectronic-reporting-air-emissions%2Felectronic-reporting-tool-ert&data=04%7C01%7CORENTK%40michigan.gov%7C1dc6d2e8d75c49431de108da17cc97a5%7Cd5fb7087377742ad966a892ef47225d1%7C0%7C0%7C637848464721189314%7CUnknown%7CTWFpbGZsb3d8eyJWIjoiMC4wLjAwMDAiLCJQIjoiV2luMzIiLCJBTiI6Ik1haWwiLCJXVCI6Mn0%3D%7C3000&sdata=2SzgJhiLTkCrz%2F%2Fmn8x%2Fa6qs8x9MqOWldPL6U1Cq%2FSo%3D&reserved=0)). Performance test data must be submitted in a file format generated through the use of the EPA's ERT or an alternate electronic file format consistent with the extensible markup language (XML) schema listed on the EPA's ERT website. For data collected using test methods not listed on the ERT Website, the permittee must submit the results of the performance test to the Administrator at the appropriate address listed in 40 CFR 63.13. **(40 CFR 63.3920(b) & (d))**
3. Initial notifications required in 40 CFR 63.9(b) and the notification of compliance status required in 40 CFR 63.9(h) and 40 CFR 63.3910(c) to the USEPA via the CEDRI. The CEDRI interface can be accessed through the EPA's CDX ([*https://cdx.epa.gov/*](https://cdx.epa.gov/)). The permittee must upload to CEDRI an electronic copy of each applicable notification in portable document format (PDF). The applicable notification must be submitted by the deadline specified in this subpart, regardless of the method in which the reports are submitted. **(40 CFR 63.3920(e))**
4. On and after January 5, 2021, or once the reporting template has been available on the CEDRI website for 1-year, whichever date is later, the semiannual compliance report required in 40 CFR 63.3920(a) to the USEPA via the CEDRI. The CEDRI interface can be accessed through the EPA's CDX ([*https://cdx.epa.gov/*](https://cdx.epa.gov/)). The permittee must use the appropriate electronic template on the CEDRI website for this subpart or an alternate electronic file format consistent with the XML schema listed on the CEDRI website ([*https://www.epa.gov/electronic-reporting-air-emissions/compliance-and-emissions-data-reporting-interface-cedri*](https://www.epa.gov/electronic-reporting-air-emissions/compliance-and-emissions-data-reporting-interface-cedri)). The date report templates become available will be listed on the CEDRI website. If the reporting form for the semiannual compliance report specific to this subpart is not available in CEDRI at the time that the report is due, the permittee must submit the report to the USEPA at the appropriate addresses listed in 40 CFR 63.13. Once the form has been available in CEDRI for 1 year begin submitting all subsequent reports via CEDRI. **(40 CFR 63.3920(f))**
	* 1. The permittee must report the results of performance tests for emission capture systems and add-on control devices within 60 days after the completion of the performance tests. The permittee shall submit any performance test reports to the AQD Technical Programs Unit and District Office in a format approved by the AQD. **(R 336.2001(5), 40 CFR 63.3920(b))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

NA

**IX. OTHER REQUIREMENT(S)**

The permittee shall comply with all applicable provisions of the National Emission Standards for Hazardous Air Pollutants for Surface Coating of Miscellaneous Metal Parts and Products. **(40 CFR Part 63, Subparts A & MMMM)**

FGRULE287(2)(c)

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Any emission unit that emits air contaminants and is exempt from the requirements of Rule 201 pursuant to Rule 278, Rule 278a and Rule 287(2)(c). Emission units installed/modified before December 20, 2016, may show compliance with Rule 287 in effect at the time of installation/modification.

**Emission Units installed on or after December 20, 2016:** None

**Emission Units installed prior to December 20, 2016:** EUSERVICE-BOOTH

**POLLUTION CONTROL EQUIPMENT**

Dry Fabric Filter

**I. EMISSION LIMIT(S)**

NA

**II. MATERIAL LIMIT(S)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Material** | **Limit** | **Time Period/Operating Scenario** | **Equipment** | **Underlying Applicable Requirement** |
| 1. Coatings
 | 200 Gallons/month(minus water as applied) | Calendar month | Each emission unit | **R 336.1287(2)(c)(i)** |

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

NA

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. Any exhaust system installed on or after December 20, 2016, that serves only coating spray equipment shall be equipped with a dry filter control or water wash control which is installed, maintained, and operated in accordance with the manufacturer’s specifications, or the permittee develops a plan which provides to the extent practicable for the maintenance and operation of the equipment in a manner consistent with good air pollution control practices for minimizing emissions. All emission units installed before December 20, 2016, with an exhaust system that serves only coating spray equipment must have a properly installed and operated particulate control system. **(R 336.1213(2), R 336.1287(2)(c)(ii), R 336.1910)**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. The permittee shall maintain records of the following information for each emission unit for each calendar month using the methods outlined in the EGLE, AQD Rule 287(2)(c), Permit to Install Exemption Record form (EQP 3562) or in a format acceptable to the AQD District Supervisor. **(R 336.1213(3))**

a. Volume of coating used, as applied, minus water, in gallons. **(R 336.1287(2)(c)(iii))**

b. Documentation of any filter replacements or maintenance of water wash control for exhaust systems serving coating spray equipment or other documentation included in a plan developed by the owner or operator of the equipment. **(R 336.1213(3))**

**See Appendix 4**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

NA

**IX. OTHER REQUIREMENT(S)**

NA

## FGCOLDCLEANERS

**FLEXIBLE GROUP CONDITIONS**

**DESCRIPTION**

Any cold cleaner that is grandfathered or exempt from Rule 201 pursuant to Rule 278, Rule 278a and Rule 281(2)(h) or Rule 285(2)(r)(iv). Existing cold cleaners were placed into operation prior to July 1, 1979. New cold cleaners were placed into operation on or after July 1, 1979.

**Emission Unit:** EUCOLDCLEANER

**POLLUTION CONTROL EQUIPMENT**

NA

**I. EMISSION LIMIT(S)**

NA

**II. MATERIAL LIMIT(S)**

1. The permittee shall not use cleaning solvents containing more than five percent by weight of the following halogenated compounds: methylene chloride, perchloroethylene, trichloroethylene, 1,1,1‑trichloroethane, carbon tetrachloride, chloroform, or any combination thereof. **(R 336.1213(2))**

**III. PROCESS/OPERATIONAL RESTRICTION(S)**

1. Cleaned parts shall be drained for no less than 15 seconds or until dripping ceases. **(R 336.1611(2)(b), R 336.1707(3)(b))**

2. The permittee shall perform routine maintenance on each cold cleaner as recommended by the manufacturer. **(R 336.1213(3))**

**IV. DESIGN/EQUIPMENT PARAMETER(S)**

1. The cold cleaner must meet one of the following design requirements:

a. The air/vapor interface of the cold cleaner is no more than ten square feet. **(R 336.1281(2)(h))**

b. The cold cleaner is used for cleaning metal parts and the emissions are released to the general in-plant environment. **(R 336.1285(2)(r)(iv))**

2. The cold cleaner shall be equipped with a device for draining cleaned parts. **(R 336.1611(2)(b), R 336.1707(3)(b))**

3. All new and existing cold cleaners shall be equipped with a cover and the cover shall be closed whenever parts are not being handled in the cold cleaner. **(R 336.1611(2)(a), R 336.1707(3)(a))**

4. The cover of a new cold cleaner shall be mechanically assisted if the Reid vapor pressure of the solvent is more than 0.3 psia or if the solvent is agitated or heated. **(R 336.1707(3)(a))**

5. If the Reid vapor pressure of any solvent used in a new cold cleaner is greater than 0.6 psia; or, if any solvent used in a new cold cleaner is heated above 120ºF, then the cold cleaner must comply with at least one of the following provisions:

a. The cold cleaner must be designed such that the ratio of the freeboard height to the width of the cleaner is equal to or greater than 0.7. **(R 336.1707(2)(a))**

b. The solvent bath must be covered with water if the solvent is insoluble and has a specific gravity of more than 1.0. **(R 336.1707(2)(b))**

c. The cold cleaner must be controlled by a carbon adsorption system, condensation system, or other method of equivalent control approved by the AQD. **(R 336.1707(2)(c))**

**V. TESTING/SAMPLING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

NA

**VI. MONITORING/RECORDKEEPING**

Records shall be maintained on file for a period of five years. **(R 336.1213(3)(b)(ii))**

1. For each new cold cleaner in which the solvent is heated, the solvent temperature shall be monitored and recorded at least once each calendar week during routine operating conditions. **(R 336.1213(3))**

2. The permittee shall maintain the following information on file for each cold cleaner: **(R 336.1213(3))**

a. A serial number, model number, or other unique identifier for each cold cleaner.

b. The date the unit was installed, manufactured or that it commenced operation.

c. The air/vapor interface area for any unit claimed to be exempt under Rule 281(2)(h).

d. The applicable Rule 201 exemption.

e. The Reid vapor pressure of each solvent used.

f. If applicable, the option chosen to comply with Rule 707(2).

3. The permittee shall maintain written operating procedures for each cold cleaner. These written procedures shall be posted in an accessible, conspicuous location near each cold cleaner. **(R 336.1611(3), R 336.1707(4))**

1. As noted in Rule 611(2)(c) and Rule 707(3)(c), if applicable, an initial demonstration that the waste solvent is a safety hazard shall be made prior to storage in non-closed containers. If the waste solvent is a safety hazard and is stored in non-closed containers, verification that the waste solvent is disposed of so that not more than 20%, by weight, is allowed to evaporate into the atmosphere shall be made on a monthly basis. **(R 336.1213(3), R 336.1611(2)(c), R 336.1707(3)(c))**

**VII. REPORTING**

1. Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. **(R 336.1213(3)(c)(ii))**

2. Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. **(R 336.1213(3)(c)(i))**

3. Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be postmarked or received by the appropriate AQD District Office by March 15 for the previous calendar year. **(R 336.1213(4)(c))**

**See Appendix 8**

**VIII. STACK/VENT RESTRICTION(S)**

NA

**IX. OTHER REQUIREMENT(S)**

NA

# E. NON-APPLICABLE REQUIREMENTS

At the time of the ROP issuance, the AQD has determined that no non-applicable requirements have been identified for incorporation into the permit shield provision set forth in the General Conditions in Part A pursuant to Rule 213(6)(a)(ii).

|  |
| --- |
| **APPENDICES** |

## Appendix 1. Acronyms and Abbreviations

|  |  |
| --- | --- |
| **Common Acronyms** | **Pollutant / Measurement Abbreviations** |
| AQD | Air Quality Division | acfm | Actual cubic feet per minute |
| BACT | Best Available Control Technology | BTU | British Thermal Unit |
| CAA | Clean Air Act | °C | Degrees Celsius |
| CAM | Compliance Assurance Monitoring | CO | Carbon Monoxide |
| CEM | Continuous Emission Monitoring | CO2e | Carbon Dioxide Equivalent |
| CEMS | Continuous Emission Monitoring System | dscf | Dry standard cubic foot |
| CFR | Code of Federal Regulations | dscm | Dry standard cubic meter |
| COM | Continuous Opacity Monitoring | °F | Degrees Fahrenheit |
| Department/department | Michigan Department of Environment, Great Lakes, and Energy | gr | Grains |
| HAP | Hazardous Air Pollutant |
| EGLE | Michigan Department of Environment, Great Lakes, and Energy | Hg | Mercury |
| hr | Hour |
| EU | Emission Unit | HP | Horsepower |
| FG | Flexible Group | H2S | Hydrogen Sulfide |
| GACS | Gallons of Applied Coating Solids | kW | Kilowatt |
| GC | General Condition | lb | Pound |
| GHGs | Greenhouse Gases | m | Meter |
| HVLP | High Volume Low Pressure\* | mg | Milligram |
| ID | Identification  | mm | Millimeter |
| IRSL | Initial Risk Screening Level | MM | Million |
| ITSL | Initial Threshold Screening Level | MW | Megawatts |
| LAER | Lowest Achievable Emission Rate | NMOC | Non-methane Organic Compounds |
| MACT | Maximum Achievable Control Technology | NOx | Oxides of Nitrogen |
| MAERS | Michigan Air Emissions Reporting System | ng | Nanogram |
| MAP | Malfunction Abatement Plan | PM | Particulate Matter |
| MSDS | Material Safety Data Sheet | PM10 | Particulate Matter equal to or less than 10 microns in diameter |
| NA | Not Applicable |
| NAAQS | National Ambient Air Quality Standards | PM2.5 | Particulate Matter equal to or less than 2.5microns in diameter |
| NESHAP | National Emission Standard for Hazardous Air Pollutants | pph | Pounds per hour |
| ppm | Parts per million |
| NSPS | New Source Performance Standards | ppmv | Parts per million by volume |
| NSR | New Source Review | ppmw | Parts per million by weight |
| PS | Performance Specification | % | Percent |
| PSD | Prevention of Significant Deterioration | psia | Pounds per square inch absolute |
| PTE | Permanent Total Enclosure | psig | Pounds per square inch gauge |
| PTI | Permit to Install | scf | Standard cubic feet |
| RACT | Reasonable Available Control Technology | sec | Seconds |
| ROP | Renewable Operating Permit | SO2 | Sulfur Dioxide |
| SC | Special Condition | TAC | Toxic Air Contaminant |
| SCR | Selective Catalytic Reduction | Temp | Temperature |
| SDS | Safety Data Sheet | THC | Total Hydrocarbons |
| SNCR | Selective Non-Catalytic Reduction | tpy | Tons per year |
| SRN | State Registration Number | µg | Microgram |
| TEQ | Toxicity Equivalence Quotient | µm | Micrometer or Micron |
| USEPA/EPA | United States Environmental Protection Agency | VOC | Volatile Organic Compounds |
| yr | Year |
| VE | Visible Emissions |  |  |

\*For HVLP applicators, the pressure measured at the gun air cap shall not exceed 10 psig.

## Appendix 2. Schedule of Compliance

The permittee certified in the ROP application that this stationary source is in compliance with all applicable requirements and the permittee shall continue to comply with all terms and conditions of this ROP. A Schedule of Compliance is not required. **(R 336.1213(4)(a), R 336.1119(a)(ii))**

## Appendix 3. Monitoring Requirements

Specific monitoring requirement procedures, methods or specifications are detailed in Part A or the appropriate Source-Wide, Emission Unit and/or Flexible Group Special Conditions. Therefore, this appendix is not applicable.

## Appendix 4. Recordkeeping

Specific recordkeeping requirement formats and procedures are detailed in Part A or the appropriate Source-Wide, Emission Unit and/or Flexible Group Special Conditions. Therefore, this appendix is not applicable.

## Appendix 5. Testing Procedures

Specific testing requirement plans, procedures, and averaging times are detailed in the appropriate Source-Wide, Emission Unit and/or Flexible Group Special Conditions. Therefore, this appendix is not applicable.

## Appendix 6. Permits to Install

The following table lists any PTIs issued, or ROP revision applications received since the effective date of the previously issued ROP No. MI-ROP-A9364-2014. Those ROP revision applications that are being issued concurrently with this ROP renewal are identified by an asterisk (\*). Those revision applications not listed with an asterisk were processed prior to this renewal.

Source-Wide PTI No MI-PTI-A9364-2014c is being reissued as Source-Wide PTI No. MI-PTI-A9364-2022.

| **Permit to Install Number** | **ROP Revision Application Number/Issuance Date** | **Description of Change** | **Corresponding Emission Unit(s) or Flexible Group(s)** |
| --- | --- | --- | --- |
| 89-05G | 201500127/October 20, 2015 | Incorporate PTI No: 89-05G. PTI No. 89-05G is for the addition of coating of plastic parts to the coating of metal parts at the facility. The same coatings are used on the plastic and metal parts. This means addition of plastic to the emission unit/flexible group description for FGAUTODIP, FGSPRAYMACHINES and FGMACTMMMM and another compliance option for facility-specific emission limits for the MACT permit conditions. | FGAUTODIPFGSPRAYMACHINESFGMACTMMMM |
| 545-96A | 201600105/September 19, 2016 | Incorporate PTI No: 545-96A. PTI No. 545-96A increases emission limits and the allowable throughput for EURBRMOLDING. | EURBRMOLDING |
| 159-17 | 201800047 / June 21, 2018 | Incorporate PTI No. 159-17, which was for a new adhesive coating line. The facility has decided to remove the turbo spray coating line, EUSPRAYMACHINE#9, concurrently with the installation of the adhesive coating line (EUROTSPRAY1). The permit application was not required to go through the public participation process. | EUROTSPRAY1FGSPRAYMACHINESFGRTOFGMACTMMMM |
| 97-19\* | NA/August 27, 2019 | Installation of a post-bond cure oven. | EURBRMOLDINGEURBRCUREOVEN |

## Appendix 7. Emission Calculations

There are no specific emission calculations to be used for this ROP. Therefore, this appendix is not applicable.

## Appendix 8. Reporting

**A. Annual, Semiannual, and Deviation Certification Reporting**

The permittee shall use EGLE, AQD, Report Certification form (EQP 5736) and EGLE, AQD, Deviation Report form (EQP 5737) for the annual, semi-annual and deviation certification reporting referenced in the Reporting Section of the Source-Wide, Emission Unit and/or Flexible Group Special Conditions. Alternative formats must meet the provisions of Rule 213(4)(c) and Rule 213(3)(c)(i), respectively, and be approved by the AQD District Supervisor.

**B. Other Reporting**

Specific reporting requirement formats and procedures are detailed in Part A or the appropriate Source-Wide, Emission Unit and/or Flexible Group Special Conditions. Therefore, Part B of this appendix is not applicable.