FGRULE287(2)(c)

FLEXIBLE GROUP CONDITIONS

Blue text is guidance or notes on the use of the template. Delete all blue text prior to issuing the final permit or submitting it with a permit application.

DESCRIPTION

Any emission unit that emits air contaminants and is exempt from the requirements of Rule 201 pursuant to Rule 278, Rule 278a and Rule 287(2)(c). Emission units installed/modified before December 20, 2016, may show compliance with Rule 287 in effect at the time of installation/modification.

Emission Units installed on or after December 20, 2016: {Enter Emission Unit names or if none, use “NA.”}

Identify Emission Units in this Flexible Group installed on/after December 20, 2016.

Emission Units installed prior to December 20, 2016: {Enter Emission Unit names or if none, use “NA.”}

Identify Emission Units in this Flexible Group installed before December 20, 2016.

Capture pertinent “Installation Date/Modification Date” information in the Emission Unit Summary Table to establish emission units as having pre or post December 20, 2016, requirements.

POLLUTION CONTROL EQUIPMENT

Identify specific control equipment used by the EU/FG. {If there is no pollution control equipment associated with the equipment, list “NA”.}

I. EMISSION LIMIT(S)

NA

II. MATERIAL LIMIT(S)

Material	Limit	Time Period/Operating Scenario	Equipment	Underlying Applicable Requirement
Coatings	200 Gallons/month (minus water as applied)	Calendar month	Each emission unit	R 336.1287(2)(c)(i)

III. PROCESS/OPERATIONAL RESTRICTION(S)

NA

IV. DESIGN/EQUIPMENT PARAMETER(S)

1.	Any exhaust system installed on or after December 20, 2016, that serves only coating spray equipment shall be equipped with a dry filter control or water wash control which is installed, maintained, and operated in accordance with the manufacturer’s specifications, or the permittee develops a plan which provides to the extent practicable for the maintenance and operation of the equipment in a manner consistent with good air pollution control practices for minimizing emissions. All emission units installed before December 20, 2016, with an exhaust system that serves only coating spray equipment must have a properly installed and operated particulate control system. (R 336.1213(2), R 336.1287(2)(c)(ii), R 336.1910)

V. TESTING/SAMPLING

Records shall be maintained on file for a period of five years. (R 336.1213(3)(b)(ii))

NA

VI. MONITORING/RECORDKEEPING

Records shall be maintained on file for a period of five years. (R 336.1213(3)(b)(ii))

1.	The permittee shall maintain records of the following information for each emission unit for each calendar month using the methods outlined in the EGLE, AQD Rule 287(2)(c), Permit to Install Exemption Record form (EQP 3562) or in a format acceptable to the AQD District Supervisor. (R 336.1213(3))

a.	Volume of coating used, as applied, minus water, in gallons. (R 336.1287(2)(c)(iii))

b.	Documentation of any filter replacements or maintenance of water wash control for exhaust systems serving coating spray equipment or other documentation included in a plan developed by the owner or operator of the equipment. (R 336.1213(3))

See Appendix 4

If the permittee chooses to use record form EQP3562 for its Rule 287(2)(c) emission unit(s), the permittee has the option of placing the form in Appendix 4 of the ROP. The latest version of the form is available on the EGLE, AQD website. The permittee is not required to include record form EQP3562 in their ROP.

VII. REPORTING

1.	Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. (R 336.1213(3)(c)(ii))

2.	Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be received by March 15 for the reporting period July 1 to December 31 and September 15 for the reporting period January 1 to June 30. (R 336.1213(3)(c)(i))

3.	Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be received by March 15 for the previous calendar year. (R 336.1213(4)(c))

See Appendix 8

VIII. STACK/VENT RESTRICTION(S)

NA

IX. OTHER REQUIREMENT(S)

NA