FG{ID}

FLEXIBLE GROUP CONDITIONS

Major Source – Existing Non-Emergency, SI >500 bhp

This template is for existing non-emergency, Spark Ignition and either a 2SLB, 4SLB or LFG RICE greater than 500 bhp (pick one and delete the rest).

If this template is being used for an ROP Reopening or Renewal, AND the MACT conditions were established in a PTI, the appropriate footnotes which reference enforceability must be added to each applicable condition in the template.

Blue text is guidance or notes on the use of the template. DELETE ALL BLUE TEXT PRIOR TO ISSUING THE FINAL PERMIT OR SUBMITTING IT WITH A PERMIT APPLICATION.

DESCRIPTION

40 CFR Part 63, Subpart ZZZZ - National Emission Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines (RICE), located at a major source of HAP emissions, existing non-emergency, spark ignition RICE greater than 500 brake hp.

Emission Unit(s): {Site Specific List of Emission Units}

POLLUTION CONTROL EQUIPMENT

(Enter Pollution Control Equipment or NA)

I. EMISSION LIMITS

NA

II. MATERIAL LIMITS

NA

III. PROCESS/OPERATIONAL RESTRICTIONS

(Enter Process/operational restrictions or NA)

IV. DESIGN/EQUIPMENT PARAMETERS

NA

V. TESTING/SAMPLING

Records shall be maintained on file for a period of five years. (40 CFR 63.6655)

NA

VI. MONITORING/RECORDKEEPING

Records shall be maintained on file for a period of five years. (40 CFR 63.6655)

NA

VII. REPORTING

Permit Staff – SC VII.1, 2, and 3, references to Rule 213 are ROP only. Remove before putting into a PTI. Renumber as appropriate.

Prompt reporting of deviations pursuant to General Conditions 21 and 22 of Part A. (R 336.1213(3)(c)(ii))

Semiannual reporting of monitoring and deviations pursuant to General Condition 23 of Part A. The report shall be received by March 15 for reporting period July 1 to December 31 and September 15 for reporting period January 1 to June 30. (R 336.1213(3)(c)(i))

Annual certification of compliance pursuant to General Conditions 19 and 20 of Part A. The report shall be received by March 15 for the previous calendar year. (R 336.1213(4)(c))

VIII. STACK/VENT RESTRICTIONS

NA

IX. OTHER REQUIREMENTS

1.	The permittee shall comply with all applicable provisions of the National Emission Standards for Hazardous Air Pollutants, as specified in 40 CFR Part 63, Subpart A and Subpart ZZZZ, for Stationary Reciprocating Internal Combustion Engines by the initial compliance date. (40 CFR 63.6595, 40 CFR Part 63, Subparts A and ZZZZ)